B.S.F. BOLTS

**Suppliers of B.S.F. (British Standard Fine), B.A. (British Association), Whitworth, UNF and UNC fasteners and related tooling.**

###### A.B.N. : 94 043 945 431

##### P.O. BOX 2023

**PARKDALE**

### VICTORIA 3195

**Phone** us anytime on **0408 056 255**

Or email us at: [sales@bsfbolts.net](mailto:sales@bsfbolts.net)

**website**: www.bsfbolts.net

**-----------------------------------------------------------------------------------------**

# CATALOG & PRICE LIST

**This is Version 114** **as at January 2023.**

## CONTENTS

|  |  |
| --- | --- |
| **ITEM** | **PAGE** |
| **Availability, codes, prices, dispatch & payment** | **3** |
| **Specifications, lengths, abbreviations, BSF & BA thread data** | **4** |
| **B.S.F. (British Standard Fine)** | **8** |
| **B.A. (British Association)** | **22** |
| **B.S.W. (British Standard Whitworth)** | **29** |
| **U.N.F. (Unified National Fine)** | **36** |
| **U.N.C. (Unified National Coarse)** | **39** |
| **U.N.8 (Unified National 8 TPI)** | **40** |
| **B.S.B. (Brass Thread)** | **41** |
| **Cycle Thread** | **41** |
| **Metric** | **42** |
| **Mixed-Thread Studs** | **42** |
| **Self-Tappers** | **42** |
| **Flat Washers** | **43** |
| **Spring Washers** | **44** |
| **Miscellaneous Washers** | **45** |
| **Clevis Pins** | **45** |
| **Split Pins** | **46** |
| **B.S.F. Taps** | **46** |
| **B.S.F. Button Dies** | **47** |
| **B.S.F. Die Nuts** | **48** |
| **B.A. Taps** | **48** |
| **B.A. Button Dies** | **48** |
| **Whitworth Taps** | **49** |
| **UNF Taps** | **49** |
| **B.S.B. (Brass Thread-26 TPI) Taps** | **50** |
| **Miscellaneous Hardware** | **50** |

**1. Availability**

Although we have nearly 2000 different items in stock, we are constantly adding new ones, so if the item you’re after isn’t here, please enquire anyway – it may be waiting to be listed, or we may be able to source it for you.

Not all items listed are available as our stock is constantly changing – please check with us for current availability.

We also stock small quantities of the following (non-coded) items. Please enquire for details.

* Slotted-head woodscrews in various gauges
* 6v and 12v vintage pattern globes
* Car and truck wheel studs and nuts
* Taper pins

**2. Code numbers** Each item has a code number. Please use code numbers when ordering, or if the item you want is not listed, an accurate description of the items and quantities required.

**3. Prices** All items have a per each price. Bulk prices may apply to some items – please enquire. Prices are subject to alteration without notice; please ask for current prices if you do not have a current list. **All prices are GST INCLUSIVE.** All prices are in AUS $.

**4. Dispatch & Payment**

**Please note that we are generally MAIL ORDER ONLY, although urgent pick-ups from our premises in Parkdale can be organized if required.**

We charge a flat rate of $5 for packing and post for small packages within Australia. Our packing and post charge is $10 for larger items, or $15 for basic Express (up to 5 kg) postage. Other postage options can be organized where needed.

We do NOT require pre-payment for sales. When you are satisfied with the items as received, please pay by direct deposit using the bank details on the invoice (preferred), or forward a cheque or postal order made out to “BSF BOLTS”, to:

PO BOX 2023

PARKDALE

VICTORIA 3195

**And now for the technical stuff…**

**5. Fastener Types and Descriptions**

|  |  |  |
| --- | --- | --- |
| A picture containing box and whisker chart  Description automatically generated | BOLT hex head, partly threaded | |
| Diagram  Description automatically generated | SETSCREW hex head, fully threaded | |
| a bDiagram  Description automatically generated | | a CAPSCREW  b COACHBOLT |
| abA picture containing text  Description automatically generated | | a GRUBSCREW  b ALLTHREAD |
| http://upload.wikimedia.org/wikipedia/commons/thumb/6/61/Screw_head_types.svg/400px-Screw_head_types.svg.png  g hDiagram  Description automatically generated | | HEAD PROFILES  a pan  b button  c round  d mushroom (truss)  e countersunk  f raised countersunk  g cheesehead  h fillister |
| a bA picture containing text, metalware, screw  Description automatically generatedc Screw Head - Hex Socket.svg | | HEAD DRIVES  a slotted  b Phillips  c socket (Allen) |
| a b cA picture containing metalware, gear  Description automatically generateddA picture containing metalware, gear, wheel  Description automatically generated  eShape  Description automatically generated f g h | | NUTS  a hex  b locknut, thin, jam, half  c slotted  d castle  e dome  f acorn  g ‘NYLOCK’ (nylon insert)  h wingnut |
| aShape, circle  Description automatically generatedbShape, circle  Description automatically generatedc A picture containing graphical user interface  Description automatically generated deA picture containing gear  Description automatically generated | | WASHERS  a flat  b spring  c square  d cup  e Thackeray (double coil) |
| aShape  Description automatically generated with medium confidence bText  Description automatically generated | | a SPLIT PIN  b CLEVIS PIN |
| ab Icon, circle  Description automatically generated c A picture containing wheel, gear  Description automatically generated | | a TAPS  b BUTTON DIE  c DIE NUT |

**6. Specifications**

All items are mild steel and unplated unless otherwise stated.

All bolts and setscrews are hexagon-headed unless otherwise stated.

“Drilled” means drilled at thread end for split pin.

All screw heads are slotted unless otherwise stated.

“NYLOCK” is used here as a generic term for nylon insert nuts, not as a brand name.

CAUTION : ALWAYS USE HIGH TENSILE FASTENERS IN CRITICAL APPLICATIONS SUCH AS BRAKES, STEERING AND SUSPENSION. GET PROFESSIONAL ADVICE ON TENSILE SPECIFICATIONS IF YOU ARE UNSURE.

**7. Lengths**

The length of all fasteners is measured from under the head to the end of the shaft. Most bolts & screws are partially threaded. If thread length is critical, please specify. “Setscrews” are fully-threaded hex-headed bolts, viz. all thread and no shank.

**8. Abbreviations**The following abbreviations are used in this catalog:  
csk = Countersunk

rcsk = Raised countersunk

hex = Hexagon

cad = cadmium plated (silver/white colour)

zincpl = zinc plated (silver colour)

zinc chrom. = zinc-chromate plated (yellow/gold colour)

HT = high tensile ie Grade 5 or above

TL = thread length

TPI = threads per inch

HSS = high speed steel

GKN - is a specific brand name

i/d = inner diameter

o/d = outer diameter

RHT = right hand thread

LHT = left hand thread

#### 9. B.S.F. thread

The B.S.F. thread form, which is a finer thread than B.S.W. (British Standard Whitworth), is found on many English cars, motorcycles, aircraft & other machinery. The pitch angle for B.S.F. is 55 degrees.

B.S.F. thread data is as follows:

|  |  |
| --- | --- |
| **DIAMETER** | **THREADS PER INCH** |
| 3/16’’ | 32 |
| 7/32” | 28 |
| ¼’’ | 26 |
| 9/32 ” | 26 |
| 5/16’’ | 22 |
| 3/8’’ | 20 |
| 7/16’’ | 18 |
| ½’’ | 16 |
| 9/16’’ | 16 |
| 5/8’’ | 14 |
| 11/16’’ | 14 |
| ¾’’ | 12 |
| 13/16” | 12 |
| 7/8’’ | 11 |
| 15/16” | 11 |
| 1’’ | 10 |
| 11/8’’ | 9 |
| 1¼’’ | 9 |
| 1½’’ | 8 |
| 1¾’’ | 7 |
| 2’’ | 7 |
| 2 ¼ ” | 6 |

**10. B.A. thread**

The B.A. (British Association) thread form is used in many applications where a fine thread on a small diameter fastener is required. It is used extensively in auto-electrical and instrument applications in earlier vehicles. The B.A. thread form is based on an earlier metric Swiss form in which the smallest size was “25” (0.25 mm diameter and 317 TPI !). The pitch angle for B.A. is 47.5 degrees.

B.A. thread data is as follows:

|  |  |  |
| --- | --- | --- |
| **B.A. NUMBER** | **DIAMETER** | **THREADS PER INCH** |
| 12 | 0.0512’’ (1.3 mm) | 90.9 |
| 11 | 0.0591’’ (1.5 mm) | 81.9 |
| 10 | 0.069’’ (1.7 mm) | 72.6 |
| 9 | 0.0748’’ (1.9 mm) | 65.1 |
| 8 | 0.087’’ (2.2 mm) | 59.1 |
| 7 | 0.0984’’ (2.5 mm) | 52.9 |
| 6 | 0.110’’ (2.8 mm) | 47.9 |
| 5 | 0.126’’ (3.2 mm) | 43.0 |
| 4 | 0.142’’ (3.6 mm) | 38.5 |
| 3 | 0.161’’ (4.1 mm) | 34.8 |
| 2 | 0.185’’ (4.7 mm) | 31.4 |
| 1 | 0.209’’ (5.3 mm) | 28.2 |
| 0 | 0.236’’ (6.0 mm) | 25.4 |

## 11. Taps and Dies – Buy or Hire !!!!!!!

We stock new top quality B.S.F. taps and dies in a wide range of sizes, including many hard-to-get fractional sizes and some left-hand threads!! See our full list below. **Do you need a B.S.F. tap or die for a once-off job ?** Why buy when for a fraction of the cost you can hire from us; we have taps and dies for hire from 3/16” up to 2 ¼” diameter, from just $5.00 per day !!!!!!!

**12. Warranties and Limitation of Liability**  
Warranties  
(I) All warranties and conditions which may be express or implied by law are hereby negatived or excluded save for those warranties and conditions which apply to contracts of sale between the seller and the purchaser by virtue of the operation of any Commonwealth or State legislation which applies to such contracts and cannot be excluded by express agreement.

(ii) The seller’s liability if any to the purchaser for any breach of condition or warranty implied by the Trade Practices Act 1974 (as amended) or the Goods Act 1958 (as amended) shall be limited to the replacement of the goods or the supply of equivalent goods in respect of which there may be a breach of any implied warranty or condition. No representation is made as to the suitability of any item for any particular purpose. There is no guarantee of the ongoing availability of any item.

Limitations of Liability  
The seller shall not be liable for any loss, damage, suits, actions, liabilities, demands, expenses or proceedings of whatever nature howsoever arising including but without limiting the generality of the foregoing loss, injury or damage whether consequential or otherwise from the acquisition, purchase, usage, sale, re-sale or disposal of the goods by the purchaser or from any other cause whatsoever.

**B.S.F. (British Standard Fine)**

**(Pitch angle 55 degrees)**

|  |  |  |  |
| --- | --- | --- | --- |
| Code | **Diameter & length** | Item | Price |
|  | **3/16” BSF** |  |  |
| 0192 | 3/16 x ¼ | Bolt – square head | 0.50 |
| 0205 | 3/16 x ¼ | Screw – roundhead - slotted | 0.50 |
| 0202 | 3/16 x 5/16 | Screw – cheesehead - slotted | 0.50 |
| 2014 | 3/16 x 5/16 | Grubscrew – Allen drive | 2.00 |
| 1728 | 3/16 x 3/8 | Screw – csk - steel | 0.50 |
| 0486 | 3/16 x ½ | Setscrew – zinc plated | 1.50 |
| 0214 | 3/16 x ½ | Screw – roundhead | 0.50 |
| 1405 | 3/16 x ½ | Screw – csk – slotted - cad plated | 0.60 |
| 0235 | 3/16 x ½ | Screw – fillister head – drilled head– cad plated | 0.40 |
| 0603 | 3/16 x ½ | Grubscrew – Allen drive – HT | 1.00 |
| 0195 | 3/16 x 9/16 | Screw – csk - zinc plated – Phillips | 0.40 |
|  |  |  |  |
|  |  |  |  |
| 0208 | 3/16 x 5/8 | Screw – roundhead – slotted with dimple – TL 3/8” | 0.40 |
| 0781 | 3/16 x 5/8 | Screw – mushhead – slotted – TL 3/8” | 0.50 |
| 0196 | 3/16 x 5/8 | Screw – mushhead – slotted – TL 1/2” | 0.50 |
| 1333 | 3/16 x ¾ | Setscrew – Grade R - zinplated | 1.50 |
| 0209 | 3/16 x ¾ | Screw – csk – Phillips | 0.40 |
| 1791 | 3/16 x ¾ | Screw – raised csk – slot - stnless | 2.00 |
| 0207 | 3/16 x 7/8 | Screw – csk – TL ½” - Phillips | 0.40 |
| 0240 | 3/16 x 7/8 | Screw – cheesehead – cad plated | 0.40 |
| 0197 | 3/16 x 7/8 | Screw – cheesehead – fillister head – drilled head | 1.00 |
| 1725 | 3/16 x 7/8 | Bolt – pass cad – TL ½” | 1.50 |
| 1542 | 3/16 x 1 | Bolt – TL ½” – cad plated | 1.00 |
| 1334 | 3/16 x 1 | Setscrew – mild - zinc plated | 2.00 |
|  |  |  |  |
| 1727 | 3/16 x 1 | Screw – mushhead – slotted – cad – head 6.8 mm | 1.50 |
| 2015 | 3/16 x 1 | Grubscrew – Allen drive | 2.40 |
| 1731 | 3/16 x 1 1/8 | Screw – csk – cad plated | 1.00 |
| 0219 | 3/16 x 1 3/8 | Screw – csk – cad plated – TL 3/8” | 0.50 |
| 0212 | 3/16 x 1 3/8 | Screw – mushroomhead – slotted – cad | 1.50 |
| 0218 | 3/16 x 1 ½ | Screw – csk – cad plated | 1.50 |
| 1613 | 3/16 x 1 ½ | Capscrew | 1.00 |
| 0213 | 3/16 x 1 ½ | Screw – roundhead (stepped) - slotted | 1.50 |
| 0211 | 3/16 x 1 5/8 | Screw – csk – zinc plated  – slotted - TL 3/8” | 1.50 |
| 1538 | 3/16 x 1 ¾ | Bolt – mild – zinc plated – TL ½” | 2.50 |
| 0217 | 3/16 x 1 ¾ | Screw – csk – cad plated – TL ¾ | 2.00 |
| 1335 | 3/16 x 2 | Setscrew – mild - zinc plated | 2.50 |
| 0220 | 3/16 x 2 | Screw – cheesehead – cad plated | 2.50 |
| 0168 | 3/16 x 2 | Stud – TL 3/8” each end | 2.00 |
| 0194 | 3/16 x 2 3/8 | Bolt – cad plated – TL ½” | 2.20 |
| 0526 | 3/16 x 2 ½ | Screw – csk – TL 1¼” -zinc plated | 2.20 |
| 0204 | 3/16 x 2 ¾ | Bolt – zinc-chromate plated  – TL ½ ” | 2.20 |
| 0198 | 3/16 x 3 | Bolt – cad plated – TL ½ “ | 2.20 |
| 0200 | 3/16 x 3 ¼ | Bolt – cad plated – TL ½ “ | 2.30 |
| 0201 | 3/16 x 3 5/8 | Bolt – cad plated – TL ½ “ | 2.50 |
| 0199 | 3/16 x 3 ¾ | Bolt – cad plated - TL ½ “ | 2.60 |
| 0173 | 3/16 x 4 ½ | Stud – TLs 1 ½“ and ¾” | 2.80 |
|  |  |  |  |
|  | **3/16” NUTS** |  |  |
| 1005 | 3/16 | Nut – plain hex – unplated | 0.60 |
| 0243 | 3/16 | Nut – plain hex – zinc plated | 0.60 |
| 0183 | 3/16 | Nut – brass | 1.50 |
| 0445 | 3/16 | Nut – nylock – brass – cad plated | 2.00 |
| 1756 | 3/16 | Nut – locknut - unplated | 1.00 |
| 1894 | 3/16 | Nut – dome - stainless | 5.00 |
|  |  |  |  |
|  | **7/32” BSF** |  |  |
| 1320 | 7/32 x 3/4 | Screw – csk – slotted - zinc plated | 4.00 |
| 1159 | 7/32 x 1 | Bolt – cad plated | 3.00 |
| 1160 | 7/32 x 3 | Bolt – cad plated | 4.00 |
|  |  |  |  |
|  | **7/32” NUTS** |  |  |
| 1161 | 7/32 | Nut – locknut – brass | 2.00 |
|  |  |  |  |
|  | **¼” BSF** |  |  |
| 2012 | ¼ x 1/4 | Grubscrew | 2.00 |
| 0275 | ¼ x 5/16 | Grubscrew | 1.00 |
| 0238 | ¼ x 3/8 | Setscrew – Grade R – zinc plt | 2.00 |
| 2016 | ¼ x 3/8 | Grubscrew – Allen drive | 1.50 |
| 1053 | ¼ x ½ | Setscrew – mild - zinc plated | 1.00 |
| 1504 | ¼ x ½ | Setscrew – Grade R – zinc plated | 1.50 |
| 1726 | ¼ x ½ | Setscrew - black | 1.50 |
| 1826 | ¼ x ½ | Setscrew - stainless | 3.80 |
| 0181 | ¼ x ½ | Screw – csk – slotted - unplated | 1.00 |
| 1539 | ¼ x ½ | Screw – csk – slotted - zinc plated | 1.50 |
| 0562 | ¼ x ½ | Screw – csk- slotted - cad pass | 0.50 |
| 1283 | ¼ x ½ | Screw – cheesehead – slotted - chromed | 2.50 |
| 1929 | ¼ X ½ | Screw – cheesehead – slotted - stainless | 3.50 |
| 1394 | ¼ x ½ | Screw – csk – slotted - brass | 1.00 |
| 2017 | ¼ x ½ | Grubscrew – Allen drive | 1.80 |
| 0972 | ¼ x 5/8 | Screw – roundhead – brass – slotted | 1.00 |
| 1371 | ¼ x 5/8 | Screw – roundhead – slotted – dimpled – zincchromate plated | 2.00 |
| 0126 | ¼ x 5/8 | Screw – mushroom head – cad plated | 1.00 |
| 1614 | ¼ x 5/8 | Capscrew – socket head - black | 1.00 |
| 1760 | ¼ x 5/8 | Screw – csk – slotted - zinc plated | 1.00 |
| 1889 | ¼ x 5/8 | Screw – csk – slotted – cad plt | 1.50 |
| 1732 | ¼ x ¾ | Bolt - unplated | 1.00 |
| 1772 | ¼ x ¾ | Bolt - HT – TL 3/8” - | 1.60 |
| 1124 | ¼ x ¾ | Setscrew – mild – zinc plated | 1.50 |
| 1281 | ¼ x ¾ | Setscrew – HT (Grade R) – zinc plated | 2.00 |
| 1066 | ¼ x ¾ | Capscrew – socket head – zinc plated | 1.00 |
| 1354 | ¼ x ¾ | Capscrew – socket head - chrome | 3.00 |
| 0128 | ¼ x ¾ | Screw – csk – slotted with dimple - zinc plated – TL ½” | 1.00 |
| 0578 | ¼ x ¾ | Screw – csk– slotted – zinc – fully threaded | 2.00 |
| 0366 | ¼ x ¾ | Screw – csk – socket head | 1.00 |
| 1188 | ¼ x ¾ | Screw – raised csk slotted – zinc plated | 2.50 |
| 0237 | ¼ x ¾ | Screw– mushhead-TL ½”- zinc-chromate | 2.00 |
| 0844 | ¼ x 7/8 | Bolt – HT | 1.00 |
| 0990 | ¼ x 7/8 | Setscrew – HT – zinc plated | 1.50 |
| 0787 | ¼ x 7/8 | Screw – cheesehead – slotted | 1.50 |
| 0406 | ¼ x 1 | Bolt – TL ¾” – zinc plated | 1.50 |
| 0814 | ¼ x 1 | Bolt - HT | 1.50 |
| 0144 | ¼ x 1 | Bolt – alloy | 1.50 |
| 0577 | ¼ x 1 | Setscrew – zinc plated – mild | 1.00 |
| 1054 | ¼ x 1 | Setscrew – HT – zinc plated | 2.00 |
| 1398 | ¼ x 1 | Setscrew – HT - black | 2.00 |
| 0560 | ¼ x 1 | Screw – csk- slotted – zinc-  fully threaded | 2.20 |
| 1890 | ¼ x 1 | Screw – csk - slotted with dimple– cad plated – TL ½” | 2.00 |
| 1794 | ¼ x 1 | Screw – raised csk – slot - steel | 3.00 |
| 0442 | ¼ x 1 | Screw – raised csk – brass | 1.00 |
| 1412 | ¼ x 1 | Screw – raised csk – slot-stainless | 3.00 |
| 0367 | ¼ x 1 | Screw – csk - socket head – black- TL 7/8” | 2.00 |
| 0408 | ¼ x 1 | Screw – roundhead – slotted - zinc plated | 2.00 |
| 0037 | ¼ x 1 | Screw – cheesehead – slotted – TL ½” - unplated | NLA |
| 1591 | ¼ x 1 | Screw – cheesehead – slotted – zinc plated | 2.50 |
| 2013 | ¼ X 1 | Screw – mushroom/brazier head – slot – full thread - cad plated | 1.20 |
| 1383 | ¼ x 1 | Capscrew – socket head – zinc plated | 1.50 |
| 1384 | ¼ x 1 | Capscrew – socket head- stainless | 2.50 |
| 2018 | ¼ x 1 | Grubscrew – Allen drive | 2.00 |
| 1977 | ¼ x 1 1/8 | Screw – mushroom head – slotted with dimple – TL ½” – cad plt | 1.50 |
| 0069 | ¼ x 1 1/8 | Bolt – TL ½” – cad plated | 1.60 |
| 1516 | ¼ x 1 1/8 | Bolt – HT – TL ½” - zincromate | 2.00 |
| 0695 | ¼ x 1 1/8 | Stud – ¼”shoulder – unplated | 1.00 |
| 1733 | ¼ x 1 1/8 | Stud – ¼” shoulder – cad plated | 3.00 |
| 0255 | ¼ x 1 1/8 | Stud – 1/8” shoulder – cad plated | 3.00 |
| 0843 | ¼ x 1 ¼ | Bolt – HT Grade R - TL ½” – zinc plated | 2.80 |
| 1359 | ¼ x 1 ¼ | Setscrew – mild – zinc plated | 1.50 |
| 1981 | ¼ X 1 ¼ | Screw – csk- slotted – zinc-  fully threaded | 2.00 |
| 0965 | ¼ x 1 ¼ | Screw –raised csk – slotted -  fully threaded | 1.50 |
| 0110 | ¼ x 1 ¼ | Screw – cheesehead – copper | 3.00 |
| 0252 | ¼ x 1 ¼ | Stud – drilled – cad plated | 3.00 |
| 0253 | ¼ x 1 ¼ | Stud – shoulder 1/8” – black | 3.00 |
| 0691 | ¼ x 1 ¼ | Stud – 1/8” shoulder – cad plated | 3.00 |
| 0254 | ¼ x 1 ¼ | Stud – wide shoulder | 3.00 |
| 1399 | ¼ x 1 ¼ | Capscrew – socket head – zinc plated | 1.50 |
| 0256 | ¼ x 1 5/16 | Stud – medium shoulder – cad plated | 2.00 |
| 0257 | ¼ x 1 5/16 | Stud – wide shoulder – cad plated | 2.00 |
| 0001 | ¼ x 1 3/8 | Bolt – cad plated – TL ¾” | 1.50 |
| 0258 | ¼ x 1 3/8 | Stud – cad plated | 3.00 |
| 1989 | ¼ x 1 3/8 | Stud - black | 3.00 |
| 1997 | ¼ x 1 3/8 | Bolt – HT – TL ¾” | 2.00 |
| 0259 | ¼ x 1 7/16 | Stud – cad plated | 3.00 |
| 1291 | ¼ x 1 ½ | Bolt – HT – zinc plated – TL ½ “ | 2.50 |
| 0075 | ¼ x 1 ½ | Bolt – HT – TL ¾” | 2.60 |
| 1917 | ¼ x 1 ½ | Bolt – HT – TL ½” - cad plated | 2.50 |
| 0054 | ¼ x 1 ½ | Setscrew - black | 2.00 |
| 1918 | ¼ x 1 ½ | Setscrew – HT - zincplated | 2.00 |
| 1028 | ¼ x 1 ½ | Screw – csk – slotted – zinc plated | 2.50 |
| 1762 | ¼ x 1 ½ | Screw – csk – slot with dimple – TL ½” - cad plated | 2.00 |
| 0352 | ¼ x 1 ½ | Screw – csk – socket head | 1.50 |
| 1400 | ¼ x 1 ½ | Capscrew – socket head – TL 1” - zinc plated | 2.00 |
| 0184 | ¼ x 1 5/8 | Bolt – TL ½ “ – small head – unplated | 1.50 |
| 1724 | ¼ X 1 5/8 | Bolt – HT – cad plated – TL ½” | 1.50 |
| 0231 | ¼ x 1 11/16 | Bolt – HT - cad plated – TL ½ “ | 1.50 |
|  |  |  |  |
| 0062 | ¼ x 1 5/8 | Screw – full thrd - mushroomhead | 1.50 |
| 0225 | ¼ x 1 ¾ | Bolt – TL ½” – unplated - seconds | 1.50 |
| 1288 | ¼ x 1 ¾ | Bolt – HT – cad plated – thin head – TL ½ “ | 1.50 |
| 0002 | ¼ x 1 ¾ | Bolt – HT – cad plated – TL ¾” | 1.50 |
| 0053 | ¼ x 1 ¾ | Setscrew – cad plated | 1.00 |
| 1391 | ¼ x 1 ¾ | Setcrew – zinc plated | 2.00 |
| 0353 | ¼ x 1 ¾ | Screw – csk – socket head | 2.00 |
| 0068 | ¼ x 1 ¾ | Screw – raised csk – TL ½” – cad plated – dimple in slot | 2.00 |
| 0261 | ¼ x 1 ¾ | Stud –TL 3/8” – cad plated | 2.00 |
| 0260 | ¼ x 1 ¾ | Stud – TL ½” – cad plated | 2.00 |
| 1401 | ¼ X 1 ¾ | Capscrew – socket head –  TL 1 1/4” - zinc plated | 2.50 |
| 0111 | ¼ x 2 | Bolt – unplated | 2.00 |
| 1060 | ¼ x 2 | Bolt – zinc-chromate – TL ½” | 2.00 |
| 0140 | ¼ x 2 | Bolt – HT - cad plated – TL ½” RO | 2.00 |
| 0058 | ¼ x 2 | Bolt – HT– cad plated – TL ½” E20 | 2.00 |
| 0407 | ¼ x 2 | Setscrew - mild – unpl | 2.00 |
| 1554 | ¼ x 2 | Setscrew – mild - zinc plated | 2.00 |
| 1734 | ¼ x 2 | Setscrew – HT - unplated | 2.50 |
| 0064 | ¼ x 2 | Setscrew – cad plated | 2.50 |
| 1286 | ¼ x 2 | Screw – csk – slotted – zinc plated | 3.00 |
| 1751 | ¼ x 2 | Screw – mushroom/brazier – slot - full thread - cad | 3.00 |
| 0003 | ¼ x 2 ¼ | Bolt – cad plated | 1.60 |
| 0004 | ¼ x 2 ¼ | Bolt – HT – cad plated – TL ½” | 1.00 |
| 0171 | ¼ x 2 ¼ | Stud – ½” thread length each end | 3.00 |
| 0082 | ¼ x 2 3/8 | Screw – raised head csk – zinc plated | 3.00 |
| 0107 | ¼ x 2 ½ | Bolt – cad plated | 2.00 |
|  |  |  |  |
| 0049 | ¼ x 2 ½ | Bolt and nut – TL ¾” | 2.00 |
| 0731 | ¼ x 2 ½ | Bolt – HT – black – TL ½ “ | 2.00 |
| 0125 | ¼ x 2 ½ | Screw – roundhead – zinc plated | 1.00 |
| 1402 | ¼ x 2 ½ | Capscrew – socket head –  TL 1 ” - zinc plated | 2.20 |
| 0005 | ¼ x 2 5/8 | Bolt – cad plated | 1.50 |
| 0113 | ¼ x 2 5/8 | Bolt | 1.50 |
| 0236 | ¼ x 2 5/8 | Bolt – drilled – unplated – TL ½” | 1.50 |
| 0365 | ¼ x 2 5/8 | Screw – roundhead | 2.00 |
| 0006 | ¼ x 2 ¾ | Bolt – TL ¾” - cad plated | 1.70 |
| 0127 | ¼ x 2 ¾ | Screw – raised csk – slotted –  TL ½” | 2.00 |
| 0170 | ¼ x 2 ¾ | Stud – TL ½” | 3.00 |
| 1403 | ¼ x 2 ¾ | Capscrew – socket head –  TL 1 “ – zinc plated | 2.50 |
| 1390 | ¼ x 2 ¾ | Capscrew – socket head –  TL 1 ¼ “ – zinc plated | 2.50 |
| 1422 | ¼ x 2 ¾ | Capscrew – socket head –  TL 1 ¼ “ – black | 2.50 |
| 0066 | ¼ x 2 7/8 | Bolt – cad plated | 2.00 |
| 0007 | ¼ x 3 | Bolt – cad plated | 2.00 |
| 0602 | ¼ x 3 | Screw – roundhead | 2.00 |
| 1695 | ¼ x 3 | Screw – csk – slot-fully threaded – cad plated | 2.00 |
| 1752 | ¼ x 3 | Screw – mush – full threaded - cad plated | 3.00 |
| 0061 | ¼ x 3 1/8 | Bolt – cad plated | 3.00 |
| 0008 | ¼ x 3 ¼ | Bolt – HT – cad plated | 3.00 |
| 0009 | ¼ x 3 ½ | Bolt – cad plated | 3.00 |
| 1204 | ¼ x 3 ½ | Screw – slotted – csk with dimple - zinc-chromate – TL ½” | 3.00 |
| 1568 | ¼ x 3 3/8 | Stud | 5.00 |
| 0010 | ¼ x 3 5/8 | Bolt – cad plated | 2.00 |
| 0226 | ¼ x 3 5/8 | Bolt – HT – TL 5/8” | 3.50 |
| 1753 | ¼ x 3 5/8 | Screw – mush-head - slot – TL ½” | 4.00 |
| 0011 | ¼ x 3 ¾ | Bolt – cad plated | 2.50 |
| 0109 | ¼ x 3 ¾ | Bolt – duralumin | 3.00 |
| 0012 | ¼ x 3 7/8 | Bolt – cad plated | 2.20 |
| 0013 | ¼ x 4 | Bolt – cad plated | 2.20 |
| 0190 | ¼ x 4 1/8 | Bolt – cad plated – TL ½” | 2.80 |
| 0154 | ¼ x 4 ¼ | Bolt – thick head | 2.50 |
| 0155 | ¼ x 4 ¼ | Bolt – thin head | 2.50 |
| 0459 | ¼ x 4 ¼ | Bolt – HT – cad plated | 2.50 |
| 0014 | ¼ x 4 ½ | Bolt – HT - cad plated | 3.20 |
| 0083 | ¼ x 4 5/8 | Bolt – TL ½” - cad plated | 3.50 |
| 0845 | ¼ x 4 ¾ | Bolt – HT – cad plated | 3.50 |
| 0065 | ¼ x 5 | Bolt - black | 3.70 |
| 0776 | ¼ x 5 | Bolt – cad plated | 4.00 |
| 0412 | ¼ x 5 ¼ | Bolt – HT | 4.70 |
| 0077 | ¼ x 5 ½ | Bolt – cad plated | 5.00 |
| 1192 | ¼ | Allthread – zinc plated | 3.00 per inch |
| 1193 | ¼ | Allthread – stainless | 4.00 per inch |
|  |  |  |  |
|  | **¼” BSF NUTS** |  |  |
| 1304 | ¼ | Nut – plain – unplated | 0.50 |
| 1178 | ¼ | Nut – plain hex – zinc plated | 0.60 |
| 0221 | ¼ | Nut – plain hex – cad plated | 0.60 |
| 0855 | ¼ | Nut – plain hex – brass | 2.00 |
| 1310 | ¼ | Nut – stainless | 2.50 |
| 1038 | ¼ | Nut – HT – cad plated | 1.00 |
| 1625 | ¼ | Nut – HT – Grade R - zinc plated | 1.50 |
| 0076 | ¼ | Nut – left hand thread – alloy | 2.00 |
| 0071 | ¼ | Nut – slotted – cad plated | 4.00 |
| 0517 | ¼ | Nut – castle – cad plated | 3.00 |
| 1755 | ¼ | Nut – castle – zinc plated | 3.00 |
| 0806 | ¼ | Nut – castle – HT | 2.50 |
| 0606 | ¼ | Dome/acorn nut – flat top | 5.00 |
| 1092 | ¼ | Dome/acorn nut – brass | 3.00 |
| 1566 | ¼ | Dome nut – chromed | 6.00 |
| 1887 | ¼ | Dome nut - stainless | 5.60 |
| 1841 | ¼ | Dome nut – 3/8” tall – round top - unplated | 4.00 |
| 0405 | ¼ | Locknut – unplated | 0.40 |
| 1338 | ¼ | Locknut – zinc plated | 0.60 |
| 1741 | ¼ | Locknut – cad plated | 2.00 |
| 1778 | ¼ | Locknut - brass | 2.50 |
| 1010 | ¼ | Locknut – left hand thread – brass | 3.00 |
| 1234 | ¼ | Nut – fibrelock – cad plated | 2.00 |
| 0685 | ¼ | Nut – nylock – zinc chromate | 2.00 |
| 1163 | ¼ | Nut – nylock – zinc plated | 2.00 |
| 0182 | ¼ | Nut – anchor – elliptic -2 holes | 2.00 |
| 0189 | ¼ | Wingnut – brass | 5.00 |
| 1280 | ¼ | Manifold nuts – brass - 5/16” deep | 3.00 |
| 0523 | ¼ | Manifold nuts – brass – 7/16” deep | 3.00 |
| 1574 | ¼ | Nut – deep (6.5 mm) | 4.00 |
| 1575 | ¼ | Nut – deep – cad plated | 4.00 |
|  |  |  |  |
|  |  |  |  |
|  | **5/16” BSF** |  |  |
| 2019 | **5/16 x 5/16** | Grubscrew – Allen drive | 1.50 |
| 0187 | 5/16 x 3/8 | Screw – cheesehead – brass – slotted | 2.00 |
| 1444 | 5/16 X 7/16 | Setscrew – HT – cad plated | 1.50 |
| 0402 | 5/16 x ½ | Setscrew – black | 1.50 |
| 1570 | 5/16 x ½ | Setscrew – HT - zinc plated | 1.50 |
| 0272 | 5/16 x ½ | Grubscrew – stainless | 1.50 |
| 0401 | 5/16 x 5/8 | Setscrew – zinc plated | 1.50 |
| 0264 | 5/16 x 5/8 | Capscrew – socket head - unplated | 2.00 |
| 1191 | 5/16 x ¾ | Setscrew – zinc plated – mild | 2.00 |
| 1662 | 5/16 x ¾ | Setscrew – HT – Grade R | 2.00 |
| 0593 | 5/16 x ¾ | Screw – csk – slotted – zinc plated | 2.00 |
| 0273 | 5/16 x ¾ | Grubscrew / Stud (Allen drive) | 2.00 |
| 0124 | 5/16 x 7/8 | Bolt – HT – TL 5/8” - cad plated | 1.50 |
| 1406 | 5/16 X 7/8 | Bolt – HT – unplated –TL 5/8” | 1.50 |
| 0133 | 5/16 x 7/8 | Bolt – alloy | 1.50 |
| 0598 | 5/16 x 7/8 | Setscrew – stainless | 2.20 |
| 1271 | 5/16 x 15/16 | Bolt – HT – TL ½” – cad plated | 2.00 |
|  | 5/16 x 1 | Bolt – HT- TL ½’ | 2.00 |
| 0853 | 5/16 x 1 | Setscrew – zinc plated – mild | 2.00 |
| 0977 | 5/16 x 1 | Setscrew – zinc plated – HT (Grade R) | 2.50 |
| 1982 | 5/16 X 1 | Setscrew – domed hex head - stainless | 9.00 |
| 0444 | 5/16 x 1 | Screw – csk – slotted – zinc plated | 2.50 |
| 1748 | 5/16 x 1 | Screw – csk – slotted - unplated | 2.00 |
| 0121 | 5/16 x 1 | Screw – cheesehead – cad plated | 2.00 |
| 1407 | 5/16 X 1 | Screw – csk – slotted – brass | 2.50 |
| 1747 | 5/16 x 1 | Screw – roundhead - unplated | 2.00 |
| 1549 | 5/16 x 1 | Capscrew - chromed | 3.20 |
| 1616 | 5/16 x 1 | Capscrew – socket head - black | 2.00 |
| 1665 | 5/16 x 1 | Screw – mushhead – slot -TL ½” | 2.00 |
| 1443 | 5/16 X 1 1/8 | Bolt – HT – TL ½” – cad plated | 1.50 |
| 1759 | 5/16 x 1 1/8 | Screw – csk – slot –TL ½” - cad | 2.00 |
| 0179 | 5/16 x 1 ¼ | Bolt - HT– cad plated – TL ½” | 2.00 |
| 1041 | 5/16 x 1 ¼ | Bolt – mild – unplated – TL 7/8” | 1.50 |
| 1535 | 5/16 x 1 ¼ | Bolt – mild – zinc plated – TL ¾” | 1.60 |
| 0138 | 5/16 x 1 ¼ | Bolt – HT –cad plated – TL ½” | 2.50 |
| 1569 | 5/16 x 1 ¼ | Bolt – HT – zinc plated – TL ½ ” | 3.00 |
| 1301 | 5/16 x 1 ¼ | Setscrew – mild – unplated | 2.00 |
| 1583 | 5/16 x 1 ¼ | Setscrew – HT - zinc plated | 2.50 |
| 0165 | 5/16 x 1 ¼ | Stud | 5.00 |
| 1346 | 5/16 x 1 ¼ | Screw – csk – socket head | 2.50 |
| 1599 | 5/16 x 1 ¼ | Capscrew – socket head – zinc plated | 1.50 |
| 1617 | 5/16 x 1 ¼ | Capscrew – socket head – fully threaded - black | 2.00 |
| 0831 | 5/16 x 1 3/8 | Bolt – TL 7/8” - cad plated | 4.50 |
| 1800 | 5/16 x 1 7/16 | Bolt – TL ½” – cad plated | 2.50 |
| 1572 | 5/16 x 1 ½ | Bolt – HT – TL 5/8” - zinc-chromate | 2.00 |
| 1361 | 5/16 x 1 ½ | Bolt – Grade R – TL 3/4” – zinc plated | 3.50 |
| 0139 | 5/16 x 1 ½ | Bolt – Grade 8.8 – TL 3/4 ” – zinc plated | 2.30 |
| 1598 | 5/16 x 1 ½ | Bolt – Grade R – TL 7/8” - zinc plated | 2.50 |
| 0403 | 5/16 x 1 ½ | Setscrew – mild – zinc plated | 2.00 |
| 1919 | 5/16 X 1 ½ | Setscrew – HT - zincplated | 2.50 |
| 0413 | 5/16 x 1 ½ | Setscrew – round knurled head – brass + knurled nut | 6.00 |
| 0518 | 5/16 x 1 ½ | Capscrew – socket head | 1.50 |
| 0443 | 5/16 x 1 ½ | Screw – csk – socket head | 1.00 |
| 1419 | 5/16 x 1 ½ | Stud – TL 3/8” + 5/8” | 4.00 |
| 0015 | 5/16 x 1 5/8 | Bolt – cad plated - HT – TL 5/8” | 5.00 |
| 0185 | 5/16 x 1 ¾ | Bolt – TL ½ - cad plated | 2.20 |
| 0070 | 5/16 x 1 ¾ | Bolt - HT - zincchromate plated | 2.00 |
| 1885 | 5/16 X 1 ¾ | Bolt – HT – cad plated | 2.50 |
| 0481 | 5/16 x 1 ¾ | Capscrew – socket head | 2.00 |
| 0480 | 5/16 x 1 ¾ | Screw – csk – socket head | 2.00 |
| 0051 | 5/16 x 1 7/8 | Bolt – cad plated – TL ½” | 2.00 |
| 0067 | 5/16 x 2 | Bolt – cad plated –HT - TL 5/8” | 2.50 |
| 1442 | 5/16 x 2 | Bolt – cad plated – TL 5/8” | 2.00 |
| 1514 | 5/16 X 2 | Stud – TL ½ and 5/8 | 4.00 |
| 1530 | 5/16 X 2 | Stud – TL ¼ and 7/8” | 4.00 |
| 1363 | 5/16 x 2 | Bolt – Grade R – zinc plated – TL ¾” | 4.00 |
| 1536 | 5/16 x 2 | Bolt – mild – zinc plated – TL 5/8” | 3.50 |
| 1801 | 5/16 X 2 | Bolt – HT – TL ½” – cad plated | 3.50 |
| 0605 | 5/16 x 2 | Setscrew - | 2.00 |
| 0020 | 5/16 x 2 | Screw – csk –slotted – zinc plated | 2.00 |
| 1696 | 5/16 x 2 | Screw – csk – slotted - unplated | 2.00 |
| 1550 | 5/16 x 2 | Capscrew - chromed | 4.50 |
| 0042 | 5/16 x 2 ¼ | Bolt – cad plated HT – TL 5/8” | 3.00 |
| 0038 | 5/16 x 2 ¼ | Bolt – HT – TL 7/8” | 2.50 |
| 0265 | 5/16 x 2 ¼ | Capscrew – socket head | 3.00 |
| 1387 | 5/16 x 2 ¼ | Stud – TL 5/8 and 1 1/8 | 3.00 |
| 1515 | 5/16 X 2 ¼ | Stud – TL ½ and 3/4 | 3.00 |
| 0100 | 5/16 x 2 3/8 | Bolt – cad plated – TL ½” | 2.00 |
| 0514 | 5/16 x 2 3/8 | Stud | 2.50 |
| 1541 | 5/16 x 2 ½ | Bolt – cad plated – TL 5/8” | 3.50 |
| 1537 | 5/16 x 2 ½ | Bolt – mild –zinc plated – TL ¾’ | 2.80 |
| 1719 | 5/16 x 2 ½ | Bolt – HT Grade 8.8 – TL ¾” – zinc plated | 3.00 |
| 0262 | 5/16 x 2 ½ | Capscrew – socket head | 3.00 |
| 1718 | 5/16 X 2 ½ | Screw – csk – TL ½” - zinc-chromate | 3.00 |
| 1779 | 5/16 x 2 9/16 | Bolt – HT – TL 5/8”- zinc-chromate | 4.60 |
| 1382 | 5/16 x 2 5/8 | Stud - TL 3/8 + ¾ - cad | 5.20 |
| 0157 | 5/16 x 2 ¾ | Bolt | 2.20 |
| 0018 | 5/16 x 2 ¾ | Bolt - HT – zincchromate plated  – TL 5/8” | 2.50 |
| 0263 | 5/16 x 2 ¾ | Capscrew – socket head | 3.00 |
| 1362 | 5/16 x 3 | Bolt – zinc plated – HT – TL 5/8” | 5.00 |
| 0024 | 5/16 x 3 | Bolt – HT – TL 7/8” – “EZ” | 4.50 |
| 0230 | 5/16 x 3 1/8 | Bolt – cad plated – TL ½” | 1.40 |
| 0162 | 5/16 x 3 ¼ | Stud | 3.50 |
| 1942 | 5/16 x 3 3/8 | Bolt – HT – cad plt – TL 5/8” | 4.20 |
| 1388 | 5/16 x 3 3/8 | Stud – TL 5/8” + ¾” | 4.20 |
| 0034 | 5/16 x 3 ¾ | Bolt – HT - cad plated – TL ½” | 4.50 |
|  |  |  |  |
| 0452 | 5/16 x 4 | Bolt – HT – cad plt – TL ½” | 6.00 |
| 1678 | 5/16 x 4 ½ | Bolt – HT – zinc-chromate – TL ½” | 5.00 |
| 0663 | 5/16 x 5 | Bolt – cad plated – TL ½” | 5.00 |
| 1180 | 5/16 x 5 | Bolt – cad plated – TL 7/8” | 5.00 |
| 0704 | 5/16 x 5 ½ | Bolt – cad plated – TL 1” | 5.00 |
|  |  |  |  |
| 1312 | 5/16 | Allthread – stainless | 5.00 p inch |
|  |  |  |  |
|  | **5/16” NUTS** |  |  |
| 0222 | 5/16 | Nut – plain hex – unplated | 0.50 |
| 0404 | 5/16 | Nut – hex – zinc plated | 1.20 |
| 1061 | 5/16 | Nut – hex – cad plated | 1.20 |
| 1624 | 5/16 | Nut – HT – EN8 - unplated | 3.00 |
| 1543 | 5/16 | Nut – hex – 8.4 mm deep - black | 2.50 |
| 1576 | 5/16 | Nut – hex – 7.9 mm deep - unpl | 2.00 |
| 1577 | 5/16 | Nut – hex – 8.0 mm deep– cad plated | 2.50 |
| 0528 | 5/16 | Nut – hex – 11/16” deep – cad plated | 1.00 |
| 0829 | 5/16 | Nut – brass | 2.00 |
| 1311 | 5/16 | Nut – stainless | 3.50 |
| 1011 | 5/16 | Nut – left hand thread – alloy | 2.00 |
| 0835 | 5/16 | Nut – slotted – zinc – 7 mm deep | 1.00 |
| 1660 | 5/16 | Nut – slotted – HT – cad – 9.7 mm deep | 2.00 |
| 0466 | 5/16 | Nut – castle - unplated | 2.50 |
| 0830 | 5/16 | Nut – castle – cad plated | 3.00 |
| 1746 | 5/16 | Nut – castle - zinc plated | 4.00 |
| 0516 | 5/16 | Nut – dome / acorn – steel | 3.50 |
| 1776 | 5/16 | Nut – dome/acorn - stainless | 7.00 |
| 1567 | 5/16 | Nut – dome – chromed – 13 mm | 6.50 |
| 0807 | 5/16 | Locknut – zinc plated | 1.00 |
| 1777 | 5/16 | Locknut – cad plated | 2.00 |
| 1799 | 5/16 | Locknut – HT - unplated | 2.00 |
| 1749 | 5/16 | Locknut - unplated | 1.00 |
| 1012 | 5/16 | Locknut – left hand thread – steel | 3.00 |
| 1013 | 5/16 | Locknut–slotted– left hand thread – alloy | 3.00 |
| 0687 | 5/16 | Nut – nylock – 9.8 d -zinc-chromate | 2.00 |
| 1750 | 5/16 | Nut – nylock- 7.56 d – zinc-chromate | 2.00 |
| 1164 | 5/16 | Nut – nylock – zinc plated | 2.50 |
| 0045 | 5/16 | Nut – split thread lock (“Aerotight’)  Shallow Type | 2.50 |
| 1273 | 5/16 | Nut – split thread lock – (“Aerotight”)  Deep Type | 2.70 |
| 0522 | 5/16 | Nut – split thread lock – HT (“Aerotight’) | 2.80 |
| 0176 | 5/16 | Wingnut | 3.00 |
| 0188 | 5/16 | Wingnut – brass | 5.00 |
| 1008 | 5/16 | Nut – anchor – red fibrelock – single tab | 4.00 |
| 1923 | 5/16 | Nut – anchor – double tab | 5.00 |
| 0999 | 5/16 | Manifold nut – brass –3/8” deep | 4.00 |
| 0524 | 5/16 | Manifold nut – brass – ½” deep | 4.00 |
|  |  |  |  |
|  | **3/8” BSF** |  |  |
| 0105 | 3/8 x 3/8 | Setscrew | 1.50 |
| 0267 | 3/8 x 3/8 | Capscrew – socket head | 2.00 |
| 2020 | 3/8 x 3/8 | Grubscrew – Allen drive | 3.20 |
| 1615 | 3/8 x ½ | Capscrew – socket head - black | 2.00 |
| 1057 | 3/8 x ½ | Setscrew – HT – black | 2.00 |
| 0159 | 3/8 x 5/8 | Bolt – cad plated | 2.00 |
| 0410 | 3/8 x ¾ | Setscrew – HT - zinc plated | 2.20 |
| 1350 | 3/8 x ¾ | Setscrew – mild – zinc plated | 2.00 |
| 0368 | 3/8 x ¾ | Capscrew – socket head | 2.50 |
| 1375 | 3/8 X ¾ | Screw – csk – socket head | 2.00 |
| 1386 | 3/8 x ¾ | Screw – csk – brass | 3.00 |
| 0841 | 3/8 x 7/8 | Bolt – HT | 2.00 |
| 0276 | 3/8 x 7/8 | Screw – csk – zinc plated | 2.00 |
| 0409 | 3/8 x 1 | Setscrew – unplated – mild | 1.00 |
| 1349 | 3/8 x 1 | Setscrew – mild – zinc plated | 3.00 |
| 1292 | 3/8 x 1 | Setscrew – HT – zinc plated | 3.50 |
| 1445 | 3/8 x 1 | Screw – csk – socket head | 2.20 |
| 1540 | 3/8 x 1 | Screw – csk – slotted - zinc plated - | 2.50 |
| 0351 | 3/8 x 1 | Capscrew – socket head – HT | 2.00 |
| 1372 | 3/8 x 1 | Bolt – HT – TL 5/8” – head ¾”across – cad plated | 2.50 |
| 1610 | 3/8 x 1 | Bolt – HT – cad – TL 5/8” | 2.00 |
| 1416 | 3/8 x 1 | Bolt – Grade R – TL ¾”-zinc plated | 2.00 |
| 0143 | 3/8 x 1 | Screw – cheesehead – cad plated | 3.00 |
| 1531 | 3/8 X 1 | Stud – brass - TL ¼ and 3/8” | 3.00 |
| 2021 | 3/8 x 1 | Grubscrew – Allen drive | 3.00 |
| 0147 | 3/8 x 1 1/8 | Setscrew – cad plated – slotted hex head | 2.00 |
| 0664 | 3/8 x 1 1/8 | Setscrew – zinc plated – Grade R | 1.00 |
| 0161 | 3/8 x 1 ¼ | Bolt – thick head | 1.00 |
| 0468 | 3/8 x 1 ¼ | Bolt – HT | 1.00 |
| 0026 | 3/8 x 1 ¼ | Bolt – HT – TL 5/8” – cad plated | 2.00 |
| 1446 | 3/8 x 1 ¼ | Screw – csk – socket head | 2.50 |
| 1909 | 3/8 X 1 ¼ | Screw – csk – slot – TL 5/8”- cad | 5.00 |
| 0025 | 3/8 x 1 3/8 | Bolt - HT – TL 5/8” | 2.00 |
| 0114 | 3/8 x 1 ½ | Bolt – HT – TL 5/8” zincchromate | 2.50 |
| 1096 | 3/8 x 1 ½ | Bolt – HT – TL 5/8” | 2.00 |
| 1920 | 3/8 x 1 ½ | Setscrew – HT - zincplated | 3.00 |
| 1903 | 3/8 x 1 ½ | Bolt – HT – TL 1” - zincplated | 3.80 |
| 1235 | 3/8 x 1 ½ | Capscrew – black – fully threaded | 2.20 |
| 2022 | 3/8 x 1 ½ | Grubscrew – Allen drive | 3.50 |
| 0027 | 3/8 x 1 5/8 | Bolt – HT – TL 5/8” | 3.00 |
| 0172 | 3/8 x 1 5/8 | Stud – TL 5/8” – ¼” shoulder – cad plated | 5.00 |
| 1397 | 3/8 x 1 ¾ | Stud | 5.00 |
| 0029 | 3/8 x 1 ¾ | Bolt – HT – TL 5/8” -zinc-chromate | 3.00 |
| 1901 | 3/8 x 1 7/8 | Bolt – TL 5/8 – cad plated | 3.00 |
| 0842 | 3/8 x 2 | Bolt and nut – stainless; TL ¾” | 4.00 |
| 0017 | 3/8 x 2 | Bolt – HT- zinc-chromate plated  – TL 5/8” | 3.50 |
| 0711 | 3/8 x 2 | Screw – csk – zinc plated | 2.50 |
| 1360 | 3/8 x 2 1/8 | Bolt – HT – unplated – TL 5/8” | 3.00 |
| 0834 | 3/8 x 2 1/8 | Bolt – HT – cad plated – TL 5/8” | 3.50 |
| 1902 | 3/8 x 2 3/8 | Bolt – HT – TL 5/8” – cad plt | 3.50 |
| 0616 | 3/8 x 2 ½ | Bolt – HT – TL ¾ “ – black GKN | 3.00 |
| 0266 | 3/8 x 2 ½ | Capscrew –socket head - TL 11/4 | 4.00 |
| 0608 | 3/8 x 2 7/8 | Bolt – HT – cad plated - TL 5/8” | 5.00 |
| 1348 | 3/8 x 3 | Setscrew – unplated | 5.00 |
| 1563 | 3/8 x 3 | Bolt – HT – TL ¾” – zinc plt | 7.50 |
| 0836 | 3/8 x 3 1/8 | Bolt – HT – TL 5/8” – cad plated | 5.00 |
| 1767 | 3/8 x 3 ½ | Bolt – HT – cad plated – TL 5/8” | 6.00 |
| 0838 | 3/8 x 4 | Bolt - HT - zincchromate plated - TL 5/8” | 6.00 |
| 0840 | 3/8 x 4 ¾ | Bolt – HT – cad plated - TL 5/8” | 6.00 |
| 0839 | 3/8 x 5 | Bolt – HT – cad plated – TL ¾” | 7.00 |
| 0837 | 3/8 x 6 1/8 | Bolt – HT – cad plated | 7.00 |
| 1183 | 3/8 | Allthread – mild steel | 2.00 per inch |
| 0520 | 3/8 | Allthread – stainless | 8.00 per inch |
|  |  |  |  |
|  | **3/8” NUTS** |  |  |
| 1299 | 3/8 | Nut – plain hex – unplated | 1.00 |
| 0241 | 3/8 | Nut – plain hex – chamfer both sides - zinc plated | 1.80 |
| 1930 | 3/8 | Nut – plain hex – chamfer one side – zinc plated | 1.80 |
| 0527 | 3/8 | Nut – hex – 0.510” deep | 0.60 |
| 1357 | 3/8 | Nut – 9.3 mm deep – black | 5.00 |
| 1578 | 3/8 | Nut – 9.3 mm deep - unplated | 4.00 |
| 1579 | 3/8 | Nut – 9.3 mm deep – cad plated | 5.00 |
| 1294 | 3/8 | Nut – plain hex – brass | 2.20 |
| 0519 | 3/8 | Nut – stainless steel | 5.00 |
| 0966 | 3/8 | Nut – HT – Grade EN8 - unplated | 3.60 |
| 0232 | 3/8 | Nut – left hand thread - cad plated | 3.00 |
| 0808 | 3/8 | Nut – slotted | 4.00 |
| 0052 | 3/8 | Nut – slotted – left hand thread – cad plated | 3.00 |
| 0467 | 3/8 | Nut – castle - unplated | 3.00 |
| 1755 | 3/8 | Nut – castle - zinc plated | 3.00 |
| 1182 | 3/8 | Nut – dome – chrome – 3/8 hi i/s | 8.00 |
| 0134 | 3/8 | Locknut – unplated | 1.00 |
| 1612 | 3/8 | Locknut - zinc plated | 2.00 |
| 1449 | 3/8 | Locknut – cad plated | 2.00 |
| 1014 | 3/8 | Locknut – left hand thread | 2.00 |
| 1184 | 3/8 | Nut – lock – HT - slotted | 3.00 |
| 0686 | 3/8 | Nut – nylock – zinc chromate plated | 1.50 |
| 0930 | 3/8 | Nut – nylock – zinc plated | 2.50 |
| 1740 | 3/8 | Nut – nylock – cad plated | 2.00 |
| 1421 | 3/8 | Nut – split-thread locknut / Philidas | 2.00 |
| 0098 | 3/8 | Wingnut – brass - unplated | 2.60 |
| 1891 | 3/8 | Wingnut – brass – cad plated | 6.00 |
| 0099 | 3/8 | Wingnut – alloy – with wire holes | 3.00 |
| 1507 | 3/8 | Wingnut – steel – roughcast | 2.00 |
| 1295 | 3/8 | Manifold nut – brass – 7/16” deep | 3.50 |
| 0525 | 3/8 | Manifold nut – brass – 5/8” deep | 3.20 |
|  |  |  |  |
|  | **7/16” BSF** |  |  |
| 1669 | 7/16 X ¾ | Setscrew – Grade R - zinc plated | 4.50 |
| 1910 | 7/16 X ¾ | Setscrew - cad | 5.50 |
| 0920 | 7/16 x 1 | Bolt – HT – cad plated | 2.50 |
| 0479 | 7/16 x 1 | Setscrew – zinc plated - mild | 4.00 |
| 0770 | 7/16 x 1 | Setscrew – HT – black | 4.00 |
| 1279 | 7/16 x 1 ¼ | Bolt – HT – TL ¾” – zinc-chromate plated | 3.00 |
| 0551 | 7/16 x 1 ¼ | Setscrew | 4.00 |
| 0599 | 7/16 x 1 ½ | Bolt – HT – TL 5/8” – | 3.00 |
| 1648 | 7/16 X 1 ½ | Setscrew – HT –black - seconds | 3.00 |
| 0072 | 7/16 x 1 ¾ | Bolt - HT – TL ¾” | 2.60 |
| 0552 | 7/16 x 2 | Bolt – TL 1” - unplated | 2.60 |
| 0822 | 7/16 x 2 | Bolt – HT – TL 7/8” | 2.80 |
| 1229 | 7/16 x 2 | Setscrew | 3.00 |
| 0135 | 7/16 x 2 ¼ | Bolt - HT – TL 5/8”-zinc-chromate | 3.00 |
| 1285 | 7/16 x 2 ¼ | Bolt - HT – TL 3/4”-cad plated | 3.00 |
| 1679 | 7/16 x 2 3/8 | Bolt – HT – cad plated – TL ¾” | 5.50 |
| 1232 | 7/16 x 2 ½ | Bolt – TL 1” - mild | 3.00 |
| 1680 | 7/16 X 2 ½ | Bolt – HT – cad plated – T.L.3/4” | 6.00 |
| 0132 | 7/16 x 2 5/8 | Bolt – mild – TL 1” | 3.00 |
| 1230 | 7/16 x 2 3/4 | Bolt – TL 1” | 3.00 |
| 1231 | 7/16 x 3 | Bolt - | 3.00 |
| 0928 | 7/16 x 3 | Bolt – HT – TL 5/8” | 6.00 |
| 0137 | 7/16 x 3 | Setscrew – HT (Grade R) | 5.00 |
| 0927 | 7/16 x 3 ¼ | Bolt – HT – TL ¾” | 5.00 |
| 0046 | 7/16 x 3 ½ | Bolt – zinc plated or black –mild -  TL 7.8” | 5.00 |
| 0414 | 7/16 x 3 ½ | Bolt - HT – TL 1 1/8” | 5.00 |
| 1958 | 7/16 X 4 | Bolt – HT – TL ¾” | 7.00 |
| 1966 | 7/16 X 4 5/8 | Bolt – HT – cad – TL ¾” | 7.00 |
| 0420 | 7/16 x 5 | Bolt | 7.00 |
| 1007 | 7/16 x 5 | Bolt – HT | 8.00 |
| 0031 | 7/16 x 6 | Bolt – HT - cad plated – TL ¾ “ | 9.00 |
| 0775 | 7/16 x 6 | Bolt – HT (Grade R)– black – TL 1” | 9.00 |
|  |  |  |  |
|  | **7/16” NUTS** |  |  |
| 0223 | 7/16 | Nut – plain hex – unplated | 2.00 |
| 1505 | 7/16 | Nut – plain hex – zinc plated | 2.20 |
| 1605 | 7/16 | Nut – plain hex – cad plated | 2.50 |
| 0601 | 7/16 | Nut – plain hex – HT – cad plated | 3.00 |
| 1016 | 7/16 | Nut – left hand thread | 4.00 |
| 1237 | 7/16 | Nut – slotted – mild – unplated | 4.50 |
| 1236 | 7/16 | Nut – slotted – mild – zinc plated | 5.00 |
| 1686 | 7/16 | Nut – slotted – mild – cad plated | 5.00 |
| 0828 | 7/16 | Nut – slotted – HT – cad plated | 5.50 |
| 1687 | 7/16 | Nut – slotted – mild – zinc-chromate | 5.00 |
| 1233 | 7/16 | Nut – castle – unplated | 3.00 |
| 0156 | 7/16 | Nut – castle – cad plated | 3.50 |
| 1018 | 7/16 | Nut – dome – zinc plated | 5.50 |
| 1742 | 7/16 | Nut – dome - chrome | 6.00 |
| 1040 | 7/16 | Locknut – zinc plated | 2.00 |
| 1754 | 7/16 | Locknut – HT – slotted – cad plated | 4.00 |
| 1015 | 7/16 | Locknut – left hand thread | 3.00 |
| 0063 | 7/16 | Locknut – left hand thread – brass | 3.00 |
| 1165 | 7/16 | Nut – nylock – zinc plated | 5.00 |
| 1932 | 7/16 | Nut – fibrelock - cadplated | 5.50 |
| 0028 | 7/16 | Nut – split thread lock  - 10.3 mm deep ( “Aerotight’) | 5.00 |
| 0122 | 7/16 | Nut – split thread lock  – 14.2 mm deep (“Aerotight’) | 5.00 |
|  |  |  |  |
|  | **½” BSF** |  |  |
| 0274 | ½ x ½ | Grubscrew | 4.00 |
| 1379 | ½ x ½ | Screw – csk – socket head | 12.00 |
| 0652 | ½ x ¾ | Screw – csk – slotted | 5.00 |
| 1313 | ½ x ¾ | Screw – csk – socket head | 10.00 |
| 1913 | ½ x ¾ | Grubscrew - black | 6.00 |
| 0103 | ½ x 7/8 | Setscrew and nut | 5.00 |
| 1224 | ½ x 1 | Setscrew – mild – unplated | 3.00 |
| 1322 | ½ x 1 | Setscrew – mild – zinc plated | 3.00 |
| 0097 | ½ x 1 | Setscrew – HT – cad plated | 3.20 |
| 1314 | ½ X 1 | Screw – csk – socket head | 12.00 |
| 1744 | ½ x 1 | Bolt – mild – cad plated | 5.00 |
| 0094 | ½ x 1 1/8 | Setscrew | 2.50 |
| 1307 | ½ x 1 1/8 | Bolt – HT – zinc-chromate | 2.50 |
| 1308 | ½ X 1 3/16 | Bolt – HT – zinc-chromate | 4.00 |
| 1309 | ½ X 1 1/4 | Bolt – HT – zinc-chromate | 4.50 |
| 1315 | ½ x 1 1/4 | Screw – csk – socket head | 10.00 |
| 1395 | ½ x 1 ¼ | Setscrew - black – Grade R | 4.50 |
| 1757 | ½ x 1 ¼ | Setscrew – unplated | 3.00 |
| 1886 | ½ x 1 ½ | Bolt – HT – cad plated | 5.00 |
| 1225 | ½ x 1 ½ | Setscrew – unplated | 3.00 |
| 1534 | ½ x 1 ½ | Setscrew – mild – zinc plated | 4.00 |
| 0561 | ½ x 1 ½ | Capscrew – socket head | 5.00 |
| 1908 | ½ X 1 ½ | Socket screw – csk – Allen drive | 8.00 |
| 1552 | ½ X 1 5/8 | Stud – bronze | 8.00 |
| 1447 | ½ x 1 3/4 | Screw – csk – socket head | 12.00 |
| 1448 | ½ x 1 ¾ | Stud – brass | 9.00 |
| 0826 | ½ x 1 7/8 | Bolt – HT – TL 5/8” | 3.00 |
| 1336 | ½ x 2 | Setscrew – mild – zinc plated | 2.50 |
| 0081 | ½ x 2 | Setscrew – HT (grade R) | 5.00 |
| 0825 | ½ x 2 1/8 | Bolt – HT – TL 5/8” | 5.00 |
| 1788 | ½ x 2 ¼ | Bolt – stainless – TL 1” | 14.00 |
| 0136 | ½ x 2 3/8 | Bolt - HT – cad plated – TL 7/8” | 5.50 |
| 0120 | ½ x 2 3/8 | Setscrew | 4.00 |
| 0145 | ½ x 2 ½ | Setscrew | 4.00 |
| 0268 | ½ x 2 ½ | Capscrew –socket head –TL 1 ½” | 4.00 |
| 1226 | ½ x 2 1/2 | Bolt – TL 1” - mild - unplated | 4.00 |
| 1985 | ½ x 2 ½ | Bolt – HT – TL ¾” – cad plated | 6.00 |
| 0773 | ½ x 2 5/8 | Bolt – HT – cad plated | 4.50 |
| 0411 | ½ x 3 | Bolt – black – TL 1 ¼” | 4.50 |
| 1652 | ½ x 3 | Bolt – “40T” T.L. 1” – plus nut- seconds | 4.00 |
| 0269 | ½ x 3 | Capscrew – socket head – unplated - TL 1 ¼” | 4.50 |
| 1562 | ½ X 3 | Capscrew – socket head – black – TL 1 ½” | 4.50 |
| 0050 | ½ x 3 ¼ | Bolt and nut | 4.50 |
| 0160 | ½ x 3 ½ | Bolt and nut | 5.50 |
| 1284 | ½ x 3 ½ | Capscrew – Unbrako – TL 1 ¾”- black | 5.50 |
| 0117 | ½ x 3 ¾ | Bolt – mild – T.L. 1” | 5.20 |
| 0270 | ½ x 3 7/8 | Capscrew – socket head | 5.20 |
| 0818 | ½ x 4 | Bolt – HT | 6.00 |
| 0813 | ½ x 4 ½ | Bolt – HT – TL 1 1/8 “ | 6.00 |
| 1895 | ½ x 4 ½ | Bolt – mild – TL 1 ¼” | 4.00 |
| 1117 | ½ x 4 ¾ | Bolt – HT – TL 7/8” – cad plated | 6.50 |
| 1441 | ½ X 4 7/8 | Bolt – HT – TL 7/8” – cad plated | 7.00 |
| 0721 | ½ x 5 | Bolt – cad plated - TL 1 1/8 “ | 7.00 |
| 0820 | ½ x 6 | Bolt – HT – TL 1”-GKN Gr R | 8.00 |
| 0595 | ½ | Allthread – stainless | 6.00 per inch |
|  |  |  |  |
|  | **½” NUTS** |  |  |
| 0224 | ½ | Nut – plain hex – unplated | 1.20 |
| 1062 | ½ | Nut – plain hex – zinc plated | 2.50 |
| 0594 | ½ | Nut – hex – stainless | 4.00 |
| 1228 | ½ | Nut – HT – black | 4.00 |
| 1622 | ½ | Nut – plain hex – cad plated | 2.00 |
| 0087 | ½ | Nut – slotted – zinc plated | 3.50 |
| 1289 | ½ | Nut – slotted – aluminium | 4.00 |
| 1073 | ½ | Nut – slotted - HT – cad plated | 2.80 |
| 1559 | ½ | Nut – slotted – unplated | 3.00 |
| 1582 | ½ | Nut – slotted – stainless | 5.00 |
| 0091 | ½ | Nut – castle – unplated | 5.00 |
| 1321 | ½ | Nut – castle – cad plated  – 14.5 mm deep | 5.00 |
| 1227 | ½ | Nut – castle – zinc plated  – 14.2 mm deep | 5.00 |
| 0597 | ½ | Nut – castle – HT – zinc plated  -14.7 mm deep | 5.00 |
| 0500 | ½ | Locknut – zinc plated – ¾” across flats | 3.00 |
| 0116 | ½ | Locknut – 13/16” across flats | 3.00 |
| 0662 | ½ | Locknut – HT – zinc-chromate | 2.50 |
| 1743 | ½ | Locknut – slotted – cad plated | 2.00 |
| 1017 | ½ | Locknut – left hand thread | 4.00 |
| 0673 | ½ | Nut – nylock | 5.00 |
| 0149 | ½ | Nut – split thread lock (“Aerotight’) zinc-chromate | 5.00 |
| 0106 | ½ | Wingnut – brass | 5.00 |
|  |  |  |  |
|  | **9/16” BSF** |  |  |
| 1525 | 9/16 X 1 | Bolt – HT – fully threaded | 5.00 |
| 0118 | 9/16 x 1 ½ | Bolt – mild – TL 1” | 4.50 |
| 1196 | 9/16 X 1 ½ | Bolt – black – Grade R – TL 1 1/8” | 4.50 |
| 0186 | 9/16 x 2 | Bolt - mild – TL 1 ¼ | 5.00 |
| 0784 | 9/16 x 2 | Bolt – HT – GKND – TL 1 1/8” | 5.50 |
| 0705 | 9/16 x 2 ½ | Bolt | 6.00 |
| 1199 | 9/16 X 3 | Bolt – black – mild – TL 1 ¼” | 6.00 |
| 1524 | 9/16 X 3 5/8 | Bolt – HT – TL 1” | 6.00 |
| 1198 | 9/16 X 4 | Bolt – black – mild – TL 1 ½” | 7.00 |
| 1197 | 9/16 X 4 | Bolt – HT – black – TL 1” | 7.50 |
| 1195 | 9/16 x 4 1/2 | Bolt – black – Grade R - TL 1 1/8” | 8.00 |
|  |  |  |  |
|  | **9/16” NUTS** |  |  |
| 1201 | 9/16 | Nut – plain hex – unplated | 4.00 |
| 0033 | 9/16 | Nut – plain hex – HT | 4.00 |
| 0055 | 9/16 | Locknut – left hand thread – brass | 5.00 |
| 0925 | 9/16 | Slotted nut | 6.00 |
| 1200 | 9/16 | Castle nut – unplated - | 6.00 |
| 1176 | 9/16 | Castle nut – cad plated | 6.50 |
| 0926 | 9/16 | Castle nut – HT - zinc plated | 6.00 |
| 0824 | 9/16 | Locknut – HT | 6.00 |
| 1202 | 9/16 | Nut – nylock | 6.00 |
|  |  |  |  |
|  | **5/8” BSF** |  |  |
| 1217 | 5/8 x 1 | Setscrew | 3.00 |
| 1376 | 5/8 x 1 | Socket screw – csk – Allen drive | 4.20 |
| 1216 | 5/8 x 1 ¼ | Setscrew | 3.00 |
| 1218 | 5/8 x 1 ½ | Setscrew | 4.00 |
| 0271 | 5/8 x 1 ½ | Capscrew – socket head | 7.00 |
| 0131 | 5/8 x 1 ¾ | Bolt – TL 1 ¼” | 4.00 |
| 1219 | 5/8 x 1 ¾ | Bolt – TL 1 3/8” | 4.00 |
| 1415 | 5/8 x 1 ¾ | Bolt – TL 1 ¼” – Brass | 5.00 |
| 1745 | 5/8 x 1 7/8 | Bolt - TL 1” - zinplated | 5.00 |
| 1220 | 5/8 x 2 | Bolt – TL 1 1/4 | 4.00 |
| 0129 | 5/8 x 2 | Bolt and nut | 5.00 |
| 1215 | 5/8 x 2 | Setscrew | 5.00 |
| 0085 | 5/8 x 2 ¼ | Bolt – TL 1” | 4.60 |
| 0698 | 5/8 x 2 ¼ | Bolt – HT | 5.00 |
| 0057 | 5/8 x 2 3/8 | Bolt – TL 1 ¼” | 5.00 |
| 0102 | 5/8 x 2 ½ | Bolt – TL 1 ¼” - unplated | 5.00 |
| 1659 | 5/8 x 2 ½ | Bolt – HT – TL 7/8” - zinc-chromate | 8.00 |
| 0242 | 5/8 x 2 ¾ | Bolt – zinc plated – TL 1 ¼ | 5.40 |
| 1222 | 5/8 x 2 ¾” | Bolt – Grade R – TL 1 ¼” | 6.00 |
| 0030 | 5/8 x 3 | Bolt – TL 1 ¼” – mild | 5.80 |
| 1214 | 5/8 x 3 | Setscrew – mild – unpl | 6.00 |
| 0078 | 5/8 x 3 3/8 | Bolt – TL 1 ¼” | 6.40 |
| 0074 | 5/8 x 3 ¾ | Bolt - TL 1 ¼” | 7.00 |
| 0152 | 5/8 x 4 | Bolt – TL 1 ½” | 5.00 |
| 0714 | 5/8 x 4 | Bolt – HT – TL 1 ¼” | 6.00 |
| 0086 | 5/8 x 4 1/8 | Bolt – TL 1 ¼” | 7.60 |
| 0151 | 5/8 x 4 ½ | Bolt – TL 1 ¼” | 8.30 |
| 1221 | 5/8 x 6 | Bolt – TL 1 ¼” | 9.00 |
|  |  |  |  |
|  | **5/8” NUTS** |  |  |
| 0044 | 5/8 | Nut – hex – 15/16 across flats = reduced | 2.00 |
| 0043 | 5/8 | Nut – hex – 1” across flats – unplated | 3.00 |
| 1223 | 5/8 | Nut – hex – 1” across flats – zinc plated | 3.00 |
| 0032 | 5/8 | Nut – HT - plain hex | 5.00 |
| 1116 | 5/8 | Slotted nut – HT – zinc plated | 5.00 |
| 1590 | 5/8 | Slotted nut – mild - zinc plated | 5.00 |
| 0016 | 5/8 | Castle nut – zinc plated | 7.50 |
| 1208 | 5/8 | Castle nut - unplated | 6.00 |
| 0833 | 5/8 | Locknut | 4.00 |
| 0175 | 5/8 | Locknut – left hand thread | 3.50 |
| 1166 | 5/8 | Nut – nylock – zinc plated | 6.00 |
| 1564 | 5/8 | Nut – Nylock – HT - stainless | 6.00 |
| 0681 | 5/8 | Nut – split thread lock (“Aerotight”) | 6.50 |
|  |  |  |  |
|  | **11/16” BSF** |  |  |
| 0130 | 11/16 | Nut – slotted – HT – cad plated | 8.00 |
| 1517 | 11/16 | Nut – plain - cad plated | 8.00 |
|  |  |  |  |
|  | **¾” BSF** |  |  |
| 1213 | ¾ x 1 1/2 | Setscrew - unplated | 8.00 |
| 0656 | ¾ x 2 | Bolt – TL 1” - unplated | 9.00 |
| 0022 | ¾ x 2 | Setscrew | 9.00 |
| 1551 | ¾ x 2 | Socket head capscrew – Unbrako – fully threaded - black | 9.00 |
| 0847 | ¾ x 4 | Bolt – TL 1 ¼” - black | 10.00 |
| 1586 | ¾ x 4 ¼ | Bolt – TL 1 ¼ - HT - zinc-chromate | 12.00 |
| 1212 | ¾ x 4 ½ | Bolt – TL 1 ½” - mild | 10.00 |
|  |  |  |  |
|  |  |  |  |
|  | **¾” NUTS** |  |  |
| 0119 | ¾ | Nut – plain hex | 9.00 |
| 0019 | ¾ | Nut – slotted – zinc plated or black | 8.00 |
| 0079 | ¾ | Locknut | 6.00 |
| 1353 | ¾ | Nut – nylock – zinc-chromate | 8.00 |
| 1385 | ¾ | Nut - brass | 8.00 |
| 1565 | ¾ | Nut – HT – zinc-chromate | 9.00 |
| 1580 | ¾ | Nut – castle - unplated | 8.00 |
| 1581 | ¾ | Nut – castle - zinc plated | 9.00 |
|  |  |  |  |
|  | **13/16” BSF** |  |  |
|  |  |  |  |
| 1518 | 13/16 | Nut – castle - cad plated | 12.00 |
|  |  |  |  |
|  | **7/8” BSF** |  |  |
| 0923 | 7/8 x 3 | Bolt – HT | 18.00 |
| 1945 | 7/8 X 3 | Setscrew - zincplated | 18.00 |
| 1946 | 7/8 x 3 | Setscrew - unplated | 15.00 |
| 1947 | 7/8 x 4 | Setscrew - zincplated | 22.00 |
| 1944 | 7/8 x 5 | Bolt – HT – TL 1 ½” - zinchromate | 25.00 |
| 1882 | 7/8 x 6 | Bolt – TL 2” | 25.00 |
| 0706 | 7/8 x 7” | Bolt – TL 1 ¾” | 28.00 |
|  |  |  |  |
|  | **7/8” NUTS** |  |  |
| 1206 | 7/8 | Nut -plain hex - unplated | 7.00 |
| 0961 | 7/8 | Nut – slotted – zinc plated | 7.00 |
| 0036 | 7/8 | Locknut - ½” deep– cad plated | 6.00 |
| 1381 | 7/8 | Nut - brass | 7.00 |
| 1207 | 7/8 | Nut - nylock | 8.00 |
| 1210 | 7/8 | Nut – Nylock – Wheelnut - RHT | 9.00 |
| 1209 | 7/8 | Nut – Nylock – Wheelnut - LHT | 9.00 |
| 0440 | 7/8 | Nut – split thread lock (“Aerotight’) – cad plated | 9.00 |
|  |  |  |  |
|  | **1” BSF** |  |  |
| 1211 | 1 x 2 | Setscrew – black – GKN – Grade R | 12.00 |
| 0846 | 1 x 3 | Bolt – TL 2” | 14.00 |
| 1337 | 1 x 4 | Setscrew – mild - zinc plated | 16.00 |
|  |  |  |  |
|  | **1” NUTS** |  |  |
| 0021 | 1 | Nut – hex – unplated | 10.00 |
| 0023 | 1 | Locknut – hex – unplated | 8.00 |
| 1287 | 1 | Locknut – hex - zinc plated | 8.00 |
|  |  |  |  |
|  | **1 1/8” BSF** |  |  |
| 1244 | 1 1/8 | Nut – plain hex – stainless | 15.00 |
| 0716 | 1 1/8 | Nut – slotted – deep | 15.00 |
|  |  |  |  |
|  | **1 ¼” BSF** |  |  |
| 1238 | 1 1/4 | Nut – plain hex | 20.00 |

**B.A. (British Association)**

**(Pitch angle 47.5 degrees)**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Code** | **B.A. number** | **Length** | **Item** | **Price** |
|  | **0 BA** |  |  |  |
| 0278 | 0 | 3/8 | Screw – csk | 0.50 |
| 0180 | 0 | 3/8 | Screw – roundhead - steel | 0.50 |
| 1453 | 0 | 3/8 | Screw – roundhead - brass | 1.00 |
| 0277 | 0 | 3/8 | Screw – cheesehead | 0.50 |
| 0701 | 0 | ½ | Screw – csk – cad plated | 0.50 |
| 0702 | 0 | ½ | Screw – roundhead - steel | 0.50 |
| 1462 | 0 | ½ | Screw – roundhead - brass | 1.00 |
| 1102 | 0 | ½ | Screw roundhead slotted - selfthread | 0.50 |
| 0688 | 0 | 5/8 | Screw – roundhead | 0.50 |
| 0651 | 0 | 5/8 | Screw – cheesehead | 0.50 |
| 1100 | 0 | ¾ | Screw – csk – slotted – zinc plated | 0.50 |
| 0720 | 0 | ¾ | Screw – roundhead - steel | 0.50 |
| 1452 | 0 | ¾ | Screw – roundhead - brass | 1.00 |
| 1037 | 0 | ¾ | Screw – cheesehead – zinc-chromate plated | 1.50 |
| 0821 | 0 | 7/8 | Screw – csk – slotted – zinc plated | 0.50 |
| 0653 | 0 | 1 | Screw – csk - slotted– cad plated | 0.50 |
| 1099 | 0 | 1 | Screw – csk – slotted – brass | 1.50 |
| 1098 | 0 | 1 | Screw – csk – Phillips – zinc plated | 0.50 |
| 0035 | 0 | 1 | Screw – roundhead – slotted –  cad pl | 0.50 |
| 0710 | 0 | 1 | Screw – cheesehead – cad plated | 0.60 |
| 1512 | 0 | 1 | Screw – cheesehead - unplated | 1.00 |
|  |  |  |  |  |
| 1101 | 0 | 1 | Screw – cheesehead – brass | 1.50 |
| 0279 | 0 | 1 ¼ | Screw – roundhead - steel | 1.50 |
| 1461 | 0 | 1 ¼ | Screw – roundhead - brass | 2.50 |
| 0369 | 0 | 1 ¼ | Screw – cheesehead | 1.50 |
| 1915 | 0 | 1 3/8 | Screw - cheesehead | 1.50 |
| 0643 | 0 | 1 ½ | Screw – roundhead – cad plated | 1.50 |
| 0644 | 0 | 1 ½ | Screw – roundhead – black | 1.50 |
| 1912 | 0 | 1 ½ | Bolt – fully threaded | 2.00 |
| 1723 | 0 | 1 ¾ | Screw – csk – slot – cad plated | 1.50 |
| 1519 | 0 | 1 ¾ | Capscrew – black – TL 1 ¼ | 1.50 |
| 1521 | 0 | 2 | Capscrew – black – TL 1” | 2.00 |
| 1455 | 0 | 3 | Screw – csk - brass | 2.00 |
| 1456 | 0 | 3 | Screw – roundhead - brass | 2.00 |
|  |  |  |  |  |
|  | **0 BA NUTS** |  |  |  |
| 0280 | 0 | - | Nut – plain hex | 0.60 |
| 0490 | 0 | - | Nut – brass | 1.00 |
| 0491 | 0 | - | Nut – brass – nickel plated | 1.00 |
| 1478 | 0 |  | Nut - stainless | 1.50 |
| 1520 | 0 |  | Nut - nylock | 1.40 |
|  |  |  |  |  |
|  | **1 BA** |  |  |  |
| 1476 | 1 | ¾ | Screw – csk – slot - stainless | 1.00 |
| 0370 | 1 | 1 | Screw – csk | 0.50 |
| 1474 | 1 | 1 | Screw – cheesehead – slotted - brass | 0.60 |
| 0774 | 1 | 1 ½ | Screw – cheesehead – cad plated | 1.00 |
|  | **1 BA NUTS** |  |  |  |
| 0281 | 1 | - | Nut – plain hex | 0.50 |
| 0771 | 1 | -- | Nut – lock | 0.30 |
| 1475 | 1 |  | Nut - brass | 1.00 |
| 1477 | 1 |  | Nut - stainless | 1.00 |
|  |  |  |  |  |
|  | **2 BA** |  |  |  |
| 1263 | 2 | 1/8 | Screw – cheesehead – large head | 0.50 |
| 0282 | 2 | ¼ | Screw – cheesehead – zinc plated | 0.50 |
| 0372 | 2 | ¼ | Screw – cheesehead – brass | 0.50 |
| 1469 | 2 | ¼ | Screw – csk - zinc plated | 0.50 |
| 0283 | 2 | 5/16 | Screw – cheesehead – zinc plated | 0.50 |
| 0649 | 2 | 3/8 | Screw – csk - slotted - zincpltd | 0.50 |
| 1127 | 2 | 3/8 | Screw – csk – slotted – nickel plated | 0.50 |
| 0377 | 2 | 3/8 | Screw – csk – Phillips | 0.30 |
| 1344 | 2 | 3/8 | Screw – csk – socket head | 1.50 |
| 0284 | 2 | 3/8 | Screw – csk – raised head | 0.60 |
| 0375 | 2 | 3/8 | Screw – roundhead – zinc plated - Slotted | 0.50 |
| 1460 | 2 | 3/8 | Screw – roundhead - brass | 1.00 |
| 0629 | 2 | 3/8 | Screw – cheesehead – cad plated | 0.50 |
| 0660 | 2 | 3/8 | Screw – cheesehead – nickel plated | 0.50 |
| 1325 | 2 | 3/8 | Screw – cheesehead – slotted - brass - unplated | 1.00 |
| 0371 | 2 | ½ | Screw – csk – unplated | 0.50 |
| 0703 | 2 | ½ | Screw – csk – zinc plated | 0.50 |
| 0286 | 2 | ½ | Screw – csk – brass - slotted | 1.00 |
| 0287 | 2 | ½ | Screw – csk – brass – Phillips | 0.60 |
| 1345 | 2 | ½ | Screw – csk – socket head | 1.00 |
| 2000 | 2 | ½ | Screw – csk – slot - stainless | 2.00 |
| 1039 | 2 | ½ | Screw – raised csk – slotted – zinc plated | 0.60 |
| 1764 | 2 | ½ | Screw – raised csk – slotted - stainless | 2.50 |
| 1118 | 2 | ½ | Screw – raised csk – Phillips | 0.50 |
| 1358 | 2 | ½ | Screw – panhead - zinc plated | 0.50 |
| 1339 | 2 | ½ | Screw – roundhead – slot - zinc | 0.50 |
| 1420 | 2 | ½ | Screw – roundhead w dimple | 1.00 |
| 1106 | 2 | ½ | Screw – mushroom head – Phillips | 0.50 |
| 0089 | 2 | ½ | Screw – cheesehead | 0.50 |
| 1330 | 2 | ½ | Screw – cheesehead - brass | 1.00 |
| 1585 | 2 | ½ | Screw – cheesehead - stainless | 1.00 |
| 1298 | 2 | ½ | Grubscrew – slotted – zinc-chromate plated | 1.00 |
| 1414 | 2 | ½ | Setscrew – Grade R – zinc plt | 2.00 |
| 1729 | 2 | 9/16 | Screw – csk – slotted – zinc plated | 0.50 |
| 0373 | 2 | 5/8 | Screw – csk – slotted - unplated | 0.50 |
| 1943 | 2 | 5/8 | Screw – csk – slotted – cad plt | 0.70 |
| 0289 | 2 | 5/8 | Screw – csk – brass | 0.60 |
| 1034 | 2 | 5/8 | Screw – raised csk – stainless steel – slotted | 1.00 |
| 0288 | 2 | 5/8 | Screw – cheesehead | 0.50 |
| 1110 | 2 | 5/8 | Screw – panhead – Phillips cad plated | 0.50 |
| 0832 | 2 | ¾ | Bolt – TL 3/8” – cad plated | 0.50 |
| 1547 | 2 | ¾ | Setscrew - stainless | 3.50 |
| 0290 | 2 | ¾ | Screw – csk – brass | 0.60 |
| 1126 | 2 | ¾ | Screw – raised csk – slotted – steel - nickelplated | 1.00 |
| 1765 | 2 | ¾ | Screw – raised csk – slotted - stainless | 2.50 |
| 1121 | 2 | ¾ | Screw – raised csk – slotted – nickel plated – selfthreading | 0.50 |
| 1125 | 2 | ¾ | Screw – raised csk – Phillips – nickelplated | 1.00 |
| 1340 | 2 | ¾ | Screw – roundhead – slot – zinc | 1.00 |
| 1332 | 2 | ¾ | Screw – cheesehead – slotted - zinc plated | 1.00 |
| 1326 | 2 | ¾ | Screw – cheesehead – slotted – brass | 2.00 |
| 1404 | 2 | ¾ | Screw – panhead – slotted – unplated | 0.30 |
| 0661 | 2 | 7/8 | Screw – csk – slotted - zinc plated | 1.00 |
| 1119 | 2 | 7/8 | Screw – raised csk – Phillips – nickel plated | 1.00 |
| 0376 | 2 | 7/8 | Screw – roundhead | 0.50 |
| 0291 | 2 | 7/8 | Screw – cheesehead – cad plated | 1.50 |
| 1511 | 2 | 7/8 | Screw – cheesehead – unplated | 1.50 |
| 1264 | 2 | 1 | Bolt – TL ½” | 1.00 |
| 1548 | 2 | 1 | Setscrew - stainless | 2.50 |
| 1738 | 2 | 1 | Setscrew – steel - zinc plated | 2.00 |
| 1240 | 2 | 1 | Screw – csk – slotted - unplated | 1.00 |
| 1120 | 2 | 1 | Screw – csk – slotted – cad plated | 0.50 |
| 0293 | 2 | 1 | Screw – csk stainless –Phillips | 1.00 |
| 1470 | 2 | 1 | Screw – csk – brass - slotted | 1.00 |
| 1169 | 2 | 1 | Screw – raised csk – slotted – cad plated – TL 3/8” | 1.00 |
| 1766 | 2 | 1 | Screw – raised csk – slotted - stainless | 2.50 |
| 1172 | 2 | 1 | Screw – raised csk – slotted – chromed | 2.00 |
| 0234 | 2 | 1 | Screw – mushhead - slotted | 0.60 |
| 0292 | 2 | 1 | Screw – cheesehead – slotted - zinc plated | 1.00 |
| 0992 | 2 | 1 | Screw – cheesehead slotted NP brass | 1.00 |
| 0993 | 2 | 1 | Screw – cheesehead – slotted - brass – 7.9 mm head | 1.00 |
| 0802 | 2 | 1 | Screw – cheesehead – slotted – brass – 8.25 mm head | 1.00 |
| 1758 | 2 | 1 3/16 | Screw – roundhead - slotted | 0.60 |
| 0697 | 2 | 1 ¼ | Screw – csk – steel - unplated | 0.30 |
| 1466 | 2 | 1 ¼ | Screw – csk - zinc plated | 0.50 |
| 1104 | 2 | 1 ¼ | Screw – csk – slotted – brass | 1.00 |
| 0693 | 2 | 1 ¼ | Screw – roundhead – slotted – brass | 1.00 |
| 0374 | 2 | 1 ¼ | Screw – cheesehead - steel | 0.60 |
| 1103 | 2 | 1 ¼ | Screw – cheesehead – brass | 1.00 |
| 0294 | 2 | 1 3/8 | Screw – csk – brass – zinc plated | 1.00 |
| 0803 | 2 | 1 3/8 | Screw – csk – raised head with dimple – cad plate – TL 3/8” | 0.60 |
| 0295 | 2 | 1 3/8 | Screw – csk – raised head – brass - cad plated | 0.60 |
| 1792 | 2 | 1 ½ | Bolt – tall head – TL ½” | 2.50 |
| 1793 | 2 | 1 ½ | Bolt – TL ½” | 2.50 |
| 0296 | 2 | 1 ½ | Screw – csk –fully threaded zinc plated | 0.60 |
| 1472 | 2 | 1 ½ | Screw – csk - brass | 0.60 |
| 0496 | 2 | 1 ½ | Screw – csk –brass –nickel plated | 0.60 |
| 0851 | 2 | 1 ½ | Screw – roundhead – unplated | 0.50 |
| 0725 | 2 | 1 ½ | Screw - roundhead – slotted - z/plated | 0.50 |
| 1468 | 2 | 1 ½ | Capscrew - black | 1.00 |
| 1671 | 2 | 1 ½ | Screw – cheesehead – zinc plated – fully threaded | 1.50 |
| 0615 | 2 | 1 7/8 | Screw – csk –slotted –cad plated – fully threaded | 0.50 |
| 0297 | 2 | 2 | Screw – csk – brass - nickel | 0.60 |
| 1150 | 2 | 2 | Screw – roundhead – brass – nickel plated | 1.00 |
| 0780 | 2 | 2 | Screw – cheesehead – zinc plated – fully threaded | 1.00 |
| 1389 | 2 | 2 | Screw - cheesehead – TL 7/8” | 1.50 |
| 1151 | 2 | 2 | Screw – cheesehead – slotted – brass | 2.00 |
| 1270 | 2 | 2 1/2 | Capscrew – TL 1 “ | 2.50 |
| 1457 | 2 | 3 | Screw – roundhead - brass | 2.00 |
| 1907 | 2 | 6 1/4 | Bolt – ½” TL - cad plt | 8.00 |
|  |  |  |  |  |
| 1621 | 2 | 12” | 2BA Mild Allthread/studding | 12.00 |
|  |  |  |  |  |
|  |  |  |  |  |
|  | **2 BA NUTS** |  |  |  |
| 0299 | 2 | --- | Nut – plain hex | 0.50 |
| 1177 | 2 | --- | Nut – brass - unplated | 0.50 |
| 1194 | 2 | --- | Nut – brass – nickel plated | 0.50 |
| 1763 | 2 | --- | Nut – steel – nickel plated | 1.00 |
| 0623 | 2 | --- | Nut – slotted – zinc plated | 0.50 |
| 0298 | 2 | --- | Nut – castle | 1.00 |
| 0489 | 2 | --- | Nut – lock – brass | 0.60 |
| 1300 | 2 | --- | Nut – Rawlnut – rubber sleeve | 0.60 |
| 0300 | 2 | --- | Nuts – mixed | 0.30 |
| 1479 | 2 |  | Nuts – square - zinc | 0.50 |
| 1553 | 2 |  | Nut – nylock - zinced | 0.60 |
| 1673 | 2 |  | Nut - stainless | 1.00 |
| 1789 | 2 |  | Nut – dome - brass | 3.00 |
| 1790 | 2 |  | Nut – dome – steel - zinc plated | 3.00 |
| 1798 | 2 |  | Nut - Aerotight | 3.00 |
|  | **3 BA** |  |  |  |
| 0378 | 3 | ¼ | Screw – cheesehead – brass | 0.60 |
| 0301 | 3 | 5/16 | Screw – csk | 0.60 |
| 1059 | 3 | 3/8 | Screw – csk – slotted – brass | 1.00 |
| 1065 | 3 | 3/8 | Capscrew – black | 1.00 |
| 0494 | 3 | ½ | Screw – csk –slotted - brass | 1.00 |
| 1306 | 3 | ½ | Screw – cheesehead - slotted | 0.60 |
| 1697 | 3 | ½ | Screw – roundhead –slot-brass | 1.00 |
| 0495 | 3 | ¾ | Screw – csk – brass | 0.60 |
| 0379 | 3 | ¾ | Screw – roundhead – brass | 0.60 |
| 1203 | 3 | ¾ | Screw – ch-h – brass - slotted | 2.00 |
| 1626 | 3 | ¾ | Screw – ch-h – steel - slotted | 1.00 |
| 1261 | 3 | 1 | Capscrew – TL 5/8” | 2.00 |
| 0302 | 3 | 1 | Screw – csk – slotted - black | 1.00 |
| 1480 | 3 | 1 | Screw – csk - brass | 1.00 |
| 1603 | 3 | 1 | Screw – cheesehead – zinc plated | 1.00 |
| 1481 | 3 | 1 | Screw – cheesehead - brass | 1.00 |
| 1693 | 3 | 1 | Screw – roundhead - brass | 1.00 |
| 1323 | 3 | 1 ¼ | Screw – cheesehead – slotted – brass - unplated | 2.00 |
| 0690 | 3 | 1 ½ | Screw – csk – slotted - brass - unplated | 1.00 |
| 1324 | 3 | 1 ½ | Screw – csk – slotted – brass – nickel plated | 1.00 |
| 0380 | 3 | 1 ½ | Screw– roundhead – slot -black | 1.00 |
| 0604 | 3 | 1 ½ | Screw – ch-h brass slotted nickel plated | 1.00 |
| 0458 | 3 | 2 | Screw – csk | 1.00 |
| 1694 | 3 | 2 | Screw – csk - brass | 1.00 |
| 1698 | 3 | 2 | Screw – cheesehead – brass - slot | 1.00 |
|  |  |  |  |  |
|  | **3 BA NUTS** |  |  |  |
| 0303 | 3 | --- | Nut – plain hex | 0.60 |
| 1173 | 3 | --- | Nut – brass | 0.50 |
| 0304 | 3 | --- | Nut – lock | 0.50 |
|  |  |  |  |  |
|  | **4 BA** |  |  |  |
| 0305 | 4 | 1/8 | Screw – Preslite head | 0.50 |
| 1347 | 4 | 1/8 | Grubscrew – socket drive | 1.00 |
| 0817 | 4 | ¼ | Setscrew | 0.30 |
| 0397 | 4 | ¼ | Screw – csk – slotted | 0.30 |
| 0492 | 4 | ¼ | Screw – csk– brass– nickel plated | 0.50 |
| 0306 | 4 | ¼ | Screw – roundhead | 0.30 |
| 0398 | 4 | ¼ | Screw – roundhead – brass-nickelpl | 0.50 |
| 1268 | 4 | ¼ | Screw – cheesehead | 0.50 |
| 1260 | 4 | 3/8 | Screw - cheesehead | 0.50 |
| 0308 | 4 | 5/16 | Screw – csk – zinc plated | 0.30 |
| 0619 | 4 | 5/16 | Screw – csk – cad plated | 0.30 |
| 0718 | 4 | 5/16 | Screw – panhead – slotted | 0.30 |
| 0676 | 4 | 5/16 | Screw – roundhead | 0.30 |
| 0307 | 4 | 5/16 | Screw – cheesehead - steel | 0.30 |
| 1417 | 4 | 5/16 | Screw – cheesehead - brass | 0.60 |
| 0388 | 4 | 3/8 | Screw – csk – zinc plated – slotted | 0.30 |
| 0400 | 4 | 3/8 | Screw – csk– brass– nickel plated | 0.60 |
| 0665 | 4 | 3/8 | Screw - panhead – zinc plated – slotted | 0.30 |
| 0309 | 4 | 3/8 | Screw – cheesehead – zinc plated | 0.50 |
| 0389 | 4 | 3/8 | Screw – cheesehead – brass – nickel plated | 0.50 |
| 1265 | 4 | 7/16 | Bolt | 0.50 |
| 1262 | 4 | ½ | Setscrew – hex head | 0.60 |
| 0395 | 4 | ½ | Screw – csk – slotted | 0.50 |
| 0312 | 4 | ½ | Screw – csk – zinc plated – slotted | 0.30 |
| 0493 | 4 | ½ | Screw – csk – brass | 0.50 |
| 0654 | 4 | ½ | Screw – csk – raised head – zinc plated | 0.30 |
| 0659 | 4 | ½ | Screw – roundhead – cad plated – slotted | 0.30 |
| 0399 | 4 | ½ | Screw – roundhead- brass-nickel plated | 0.60 |
| 1700 | 4 | ½ | Screw – roundhead- brass | 0.50 |
| 0311 | 4 | ½ | Screw – cheesehead – zinc plated | 0.60 |
| 0310 | 4 | ½ | Screw – cheesehead – brass | 0.60 |
| 0396 | 4 | ½ | Screw – cheesehead – brass-nickel plated | 0.60 |
| 0313 | 4 | 5/8 | Screw – csk | 0.30 |
| 0393 | 4 | 5/8 | Screw – roundhead – brass | 0.60 |
| 1122 | 4 | 5/8 | Screw – cheesehead – steel – zinc plated | 0.50 |
| 0392 | 4 | 5/8 | Screw – cheesehead – brass | 0.60 |
| 0314 | 4 | ¾ | Screw – csk – zinc plated | 0.60 |
| 0692 | 4 | ¾ | Screw – roundhead – steel, cad plated | 0.60 |
| 0684 | 4 | ¾ | Screw – roundhead – brass | 1.00 |
| 1463 | 4 | ¾ | Screw – cheesehead – slotted – steel - unplated | 0.50 |
| 0315 | 4 | ¾ | Screw – cheesehead – slotted – zinc plated | 0.50 |
| 1329 | 4 | ¾ | Screw – cheesehead – slot - brass | 0.60 |
| 1413 | 4 | ¾ | Screw – csk – slotted - brass | 1.00 |
| 1508 | 4 | ¾ | Bolt – hex – steel - unplated | 1.50 |
| 1266 | 4 | 7/8 | Screw – ch-h – fully threaded | 0.50 |
| 0316 | 4 | 1 | Screw – csk – zinc plated | 0.50 |
| 0655 | 4 | 1 | Screw – csk – cad plated | 0.50 |
| 1482 | 4 | 1 | Screw – csk - brass | 0.60 |
| 0918 | 4 | 1 | Screw – roundhead slotted – cad plated | 0.50 |
| 1702 | 4 | 1 | Screw – roundhead - brass | 1.00 |
| 1465 | 4 | 1 | Screw – roundhead – slotted - zinc plated | 0.50 |
| 1464 | 4 | 1 | Screw – cheesehead – steel - unplated | 0.50 |
| 0317 | 4 | 1 | Screw – cheesehead – nickel plated | 0.50 |
| 0390 | 4 | 1 | Screw – cheesehead – brass | 0.60 |
| 1509 | 4 | 1 | Bolt – hex – steel - unplated | 1.40 |
| 1998 | 4 | 1 | Bolt – hex – steel – zincplated with nut | 2.00 |
| 1269 | 4 | 1 ¼ | Capscrew – TL 7/8” | 1.00 |
| 0674 | 4 | 1 ¼ | Screw – csk – nickel plated | 0.50 |
| 1396 | 4 | 1 ¼ | Screw – csk – fully threaded - black | 0.60 |
| 0709 | 4 | 1 ¼ | Screw – roundhead – zinc plated | 0.50 |
| 1529 | 4 | 1 ¼ | Screw – cheesehead - brass | 1.00 |
| 0707 | 4 | 1 3/8 | Screw – csk – brass | 0.60 |
| 0624 | 4 | 1 ½ | Screw – csk | 0.50 |
| 0318 | 4 | 1 ½ | Screw – csk – brass | 0.60 |
| 0849 | 4 | 1 ½ | Screw – roundhead - unplated | 0.50 |
| 0394 | 4 | 1 ½ | Screw – roundhead – brass | 0.50 |
| 1272 | 4 | 1 ½ | Screw – roundhead – brass – deep head | 0.50 |
| 1123 | 4 | 1 ½ | Screw – cheesehead – zinc plated | 0.50 |
| 1705 | 4 | 1 ½ | Screw – cheesehead - brass | 1.00 |
| 0648 | 4 | 1 ¾ | Screw – roundhead - cad plated | 0.50 |
| 0621 | 4 | 1 ¾ | Screw – roundhead – brass | 0.50 |
| 1618 | 4 | 1 7/8 | Screw – raised csk – TL ½ ” – cad plated | 0.50 |
| 0391 | 4 | 2 | Screw – csk – black | 0.50 |
| 0668 | 4 | 2 | Screw – csk – cad plated | 0.50 |
| 1458 | 4 | 2 | Screw – csk - brass | 1.00 |
| 0848 | 4 | 2 | Screw – roundhead – zinc plated | 0.50 |
| 1699 | 4 | 2 | Screw – roundhead - brass | 1.00 |
| 0719 | 4 | 2 | Screw – cheesehead – zinc plated | 0.50 |
| 1701 | 4 | 2 | Screw – cheesehead - brass | 1.00 |
| 0618 | 4 | 2 ½ | Screw – csk | 0.50 |
| 0723 | 4 | 2 ½ | Screw – cheesehead | 0.50 |
| 0708 | 4 | 3 | Screw – csk – cad plated | 0.50 |
| 0689 | 4 | 3 | Screw – cheesehead | 0.60 |
|  |  |  |  |  |
| 1620 | 4 | 12” | 4BA Mild Allthread / studding | 12.00 |
|  |  |  |  |  |
|  | **4 BA NUTS** |  |  |  |
| 0319 | 4 | ---- | Nut – plain hex – zinc plated | 0.50 |
| 1174 | 4 | --- | Nut – brass | 0.50 |
| 0320 | 4 | ---- | Nut – brass – nickel plated | 0.50 |
| 0322 | 4 | --- | Nut – lock | 0.50 |
| 0321 | 4 | --- | Rootnut | 0.50 |
|  |  |  |  |  |
|  | **5 BA** |  |  |  |
| 0677 | 5 | 1/8 | Screw- cheesehead- brass- nickel plated | 0.50 |
| 0666 | 5 | ¼ | Screw – panhead – cad plated – slotted | 0.50 |
|  |  |  |  |  |
| 1267 | 5 | ¼ | Screw - roundhead | 0.50 |
| 0323 | 5 | ½ | Screw – csk - unplated | 0.30 |
| 1990 | 5 | ½ | Screw – csk – slot – nickel plt | 0.80 |
| 1708 | 5 | ½ | Screw – csk - brass | 0.50 |
| 1914 | 5 | ½ | Screw - cheesehead | 0.50 |
| 0324 | 5 | ¾ | Screw – cheesehead | 0.50 |
| 2001 | 5 | ¾ | Setscrew – steel - unplt | 2.00 |
| 1483 | 5 | 1 | Screw – cheesehead - brass | 0.60 |
| 1704 | 5 | 1 | Screw – roundhead - brass | 0.60 |
| 1706 | 5 | 1 | Screw – csk - brass | 1.00 |
| 2002 | 5 | 1 | Setscrew – steel - unplt | 2.50 |
| 1703 | 5 | 1 ½ | Screw – roundhead- brass | 0.60 |
| 1707 | 5 | 1 ½ | Screw – csk - brass | 1.00 |
| 0617 | 5 | 2 | Screw – cheesehead – brass – nickel plated | 1.00 |
|  | **5 BA NUTS** |  |  |  |
| 0512 | 5 | --- | Nut – plain hex – steel - zinc plated | 0.30 |
| 1175 | 5 | --- | Nut – brass - unplated | 0.50 |
| 0325 | 5 | --- | Nut – brass – nickel plated | 0.50 |
|  |  |  |  |  |
|  | **6 BA** |  |  |  |
| 0326 | 6 | 3/16 | Screw – csk | 0.30 |
| 0658 | 6 | 3/16 | Screw – roundhead | 0.30 |
| 1473 | 6 | 3/16 | Screw – cheesehead - zinc plated | 0.50 |
| 0327 | 6 | ¼ | Screw – csk | 0.30 |
| 0386 | 6 | ¼ | Screw – roundhead-brass-nickel plated | 0.50 |
| 0383 | 6 | ¼ | Screw – cheesehead – brass | 0.50 |
| 1904 | 6 | ¼ | Setscrew - brass | 1.50 |
|  |  |  |  |  |
| 0675 | 6 | 3/8 | Screw – csk – steel – cad plated | 0.30 |
| 0680 | 6 | 3/8 | Screw – csk – steel – nickel plated | 0.30 |
| 0667 | 6 | 3/8 | Screw – csk – brass | 0.30 |
| 0819 | 6 | 3/8 | Screw – roundhead – zinc plated | 0.30 |
| 0627 | 6 | 3/8 | Screw – roundhead – cad plated | 0.30 |
| 0384 | 6 | 3/8 | Screw – roundhead – nickel plated | 0.30 |
| 0387 | 6 | 3/8 | Screw – cheesehead – brass | 0.50 |
| 0329 | 6 | ½ | Screw – csk – zinc plated | 0.30 |
| 0451 | 6 | ½ | Screw – roundhead – unplated | 0.30 |
| 0330 | 6 | ½ | Screw – roundhead – cad plated | 0.30 |
| 1331 | 6 | ½ | Screw – cheesehead – brass | 0.60 |
| 1471 | 6 | ½ | Screw – cheesehead – zinc plated | 0.60 |
| 1688 | 6 | ½ | Screw – csk – brass – slot | 0.60 |
| 0331 | 6 | 5/8 | Screw – csk | 0.30 |
| 0696 | 6 | 5/8 | Screw – roundhead – cadlplated | 0.30 |
| 0332 | 6 | 5/8 | Screw – roundhead – nickelplated | 0.30 |
| 0333 | 6 | ¾ | Screw – csk | 0.30 |
| 1689 | 6 | ¾ | Screw – csk – brass | 0.50 |
| 0334 | 6 | ¾ | Screw – roundhead | 0.30 |
| 1467 | 6 | ¾ | Screw – cheesehead – steel unplated | 0.50 |
| 0815 | 6 | ¾ | Screw – cheesehead - zinpt | 0.50 |
| 1328 | 6 | ¾ | Screw – cheesehead – brass | 0.60 |
| 0657 | 6 | 7/8 | Screw – csk – zinc plated | 0.30 |
| 0626 | 6 | 7/8 | Screw – roundhead – zinc plated | 0.30 |
| 0679 | 6 | 1 | Screw – csk – unplated | 0.30 |
| 0336 | 6 | 1 | Screw – csk – zinc plated | 0.30 |
| 0732 | 6 | 1 | Screw – csk – brass | 0.50 |
| 0337 | 6 | 1 | Screw – panhead | 0.30 |
| 0726 | 6 | 1 | Screw – roundhead – steel | 0.30 |
| 0722 | 6 | 1 | Screw – roundhead – brass | 0.50 |
| 0620 | 6 | 1 | Screw – roundhead – brass- nickel plated | 0.30 |
| 0335 | 6 | 1 | Screw – cheesehead – brass | 0.50 |
| 0338 | 6 | 1 | Screw – cheesehead | 0.30 |
| 0622 | 6 | 1 ½ | Screw – csk | 0.30 |
| 0339 | 6 | 1 ½ | Screw – csk – zinc plated | 0.30 |
| 0625 | 6 | 1 ½ | Screw – csk – cad plated | 0.30 |
| 0340 | 6 | 1 ½ | Screw – cheesehead – zinc plated | 0.30 |
| 1691 | 6 | 1 ½ | Screw – cheesehead – brass | 0.50 |
| 1690 | 6 | 1 ½ | Screw – roundhead – brass - | 0.50 |
| 1692 | 6 | 1 ½ | Screw – csk – brass | 0.50 |
| 1928 | 6 | 2 | Screw – csk – brass | 1.00 |
| 0724 | 6 | 2 ½ | Screw – cheesehead | 0.30 |
| 1454 | 6 | 2 ½ | Screw – csk – slotted – brass | 1.00 |
| 0682 | 6 | 3 | Screw – roundhead – brass | 0.50 |
|  |  |  |  |  |
|  | **6 BA NUTS** |  |  |  |
| 0341 | 6 | --- | Nut - plain hex | 0.30 |
| 0342 | 6 | --- | Nut – brass - unplated | 0.30 |
| 0385 | 6 | --- | Nut – brass – nickel plated | 0.30 |
|  |  |  |  |  |
|  | **7 BA** |  |  |  |
| 0344 | 7 | 3/16 | Screw – csk – brass | 0.50 |
| 0343 | 7 | 3/16 | Screw – csk – brass- nickel plated | 0.50 |
| 0328 | 7 | 5/16 | Screw – csk - black | 0.50 |
| 1067 | 7 | 3/8 | Screw – cheesehead slotted brass | 0.50 |
|  |  |  |  |  |
| 1987 | 7 | ½ | Screw – cheesehead - steel | 0.60 |
| 1486 | 7 | ½ | Screw – cheesehead - brass | 0.60 |
| 1711 | 7 | ½ | Screw – roundhead - brass | 0.60 |
| 1485 | 7 | ¾ | Screw – csk – brass – nickel plated | 0.60 |
| 1068 | 7 | 1 | Screw – cheesehead slotted brass | 0.60 |
| 1709 | 7 | 1 | Screw – roundhead - brass | 1.00 |
| 1710 | 7 | 1 | Screw – csk - brass | 1.00 |
| 2004 | 7 | 2 | Screw – roundhead – slot – nickel plated | 1.50 |
|  | **7 BA NUTS** |  |  |  |
| 0488 | 7 | --- | Nut – brass - unplated | 0.60 |
| 1484 | 7 |  | Nut – brass - zinc plated | 1.00 |
|  |  |  |  |  |
|  | **8 BA** |  |  |  |
| 0382 | 8 | ¼ | Screw – roundhead | 0.30 |
| 0345 | 8 | 3/8 | Screw – csk | 0.30 |
| 0346 | 8 | 3/8 | Screw – roundhead - steel | 0.30 |
| 1459 | 8 | 3/8 | Screw – roundhead - brass | 0.60 |
| 0347 | 8 | ½ | Screw – cheesehead – steel zinc plated | 0.30 |
| 1714 | 8 | ½ | Screw – roundhead - brass | 0.50 |
| 1487 | 8 | ½ | Screw – cheesehead - brass | 0.60 |
| 0381 | 8 | ½ | Screw – cheesehead – brass | 0.60 |
| 0348 | 8 | 5/8 | Screw – csk | 0.30 |
| 0349 | 8 | 5/8 | Screw – cheesehead | 0.30 |
| 1488 | 8 | ¾ | Screw – csk – brass – nickel plated | 0.60 |
| 1717 | 8 | ¾ | Screw – csk - brass | 1.00 |
| 0350 | 8 | 1 | Screw – cheesehead – brass | 1.00 |
| 1712 | 8 | 1 | Screw – roundhead - brass | 1.00 |
| 1713 | 8 | 1 | Screw – csk - brass | 1.00 |
| 1342 | 8 | 1 ¼ | Screw – cheesehead – brass | 1.50 |
|  | **8 BA NUTS** |  |  |  |
| 0487 | 8 | --- | Nut – brass | 0.50 |
|  | **9 BA** |  |  |  |
| 1715 | **9** | ¾ | Screw – roundhead - brass | 1.00 |
| 1489 | 9 | 1 | Screw – roundhead - brass | 1.00 |
| 1491 | 9 | 1 | Screw – cheesehead - steel | 1.00 |
| 1716 | 9 | 1 | Screw – cheesehead - brass | 1.30 |
|  |  |  |  |  |
|  | **9BA NUTS** |  |  |  |
| 1490 | **9** |  | Nuts - steel | 0.60 |
|  |  |  |  |  |
|  | **10 BA** |  |  |  |
| 1327 | 10 | 1 | Screw – cheesehead - brass | 1.50 |
| 1492 | 10 | 1 | Screw – cheesehead - steel | 1.00 |
|  | **10BA NUTS** |  |  |  |
| 1064 | 10 | -- | Nut – brass | 1.00 |
|  | **11 BA** |  |  |  |
|  |  |  |  |  |
| 1493 | **11** | ¾ | Screw – roundhead – brass nickel plated | 1.00 |
|  |  |  |  |  |
|  | **11BA NUTS** |  |  |  |
| 1351 | 11 |  | Nut - brass | 1.00 |
|  |  |  |  |  |
|  | **12 BA** |  |  |  |
| 1343 | 12 | 1 | Screw – roundhead - brass | 1.00 |
|  | **12BA NUTS** |  |  |  |
| 1352 | 12 |  | Nut – brass - | 1.00 |

**B.S.W. (British Standard Whitworth)**

**(Pitch angle 55 degrees)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Code** | **Diameter & length** | **Item** | **Price** |
|  | **1/8” WHIT** |  |  |
| 1969 | 1/8 x ¼ | Screw – roundhead – slot - | 0.50 |
| 1418 | 1/8 x 1/2 | Screw – roundhead – brass - slot | 1.00 |
| 1844 | 1/8 x 1/2 | Screw – roundhead – slot - unplated | 0.30 |
| 1851 | 1/8 x 1/2 | Screw – csk – slot - unplated | 0.30 |
| 1676 | 1/8 x 5/8 | Screw – csk – slot - stainless | 0.50 |
| 1663 | 1/8 x 3/4 | Screw – csk – slot – steel - unplated | 0.30 |
| 1852 | 1/8 x 3/4 | Screw – roundhead – slot - unplated | 0.30 |
| 1684 | 1/8 x 3/4 | Screw – steel – roundhead - slotted | 0.50 |
| 1845 | 1/8 x 1 | Screw – csk – slot - unplated | 0.50 |
| 1664 | 1/8 x 1 | Screw – csk- slot -stainless | 0.30 |
| 1846 | 1/8 x 1 | Screw – roundhead – slot - unplated | 0.50 |
| 1770 | 1/8 x 1 ¼ | Screw – roundhead- slot - steel | 0.30 |
| 1152 | 1/8 x 1 ½ | Screw- roundhead – slotted - zinc plated | 0.30 |
| 1843 | 1/8 x 1 ½ | Screw – roundhead – slot - unplated | 0.30 |
| 0504 | 1/8 x 1 ¾ | Screw – roundhead - brass | 0.50 |
| 1771 | 1/8 x 1 ¾ | Screw – roundhead- slot - steel | 0.30 |
| 1149 | 1/8 x 2 | Screw – csk - unplated | 0.30 |
| 1847 | 1/8 x 2 | Screw – csk - zinc plated | 0.50 |
| 1153 | 1/8 x 2 | Screw – roundhead – slotted | 0.30 |
| 0505 | 1/8 x 2 | Screw – cheesehead – brass | 0.50 |
| 0506 | 1/8 x 2 ½ | Screw – csk – brass | 0.50 |
| 0507 | 1/8 x 3 | Screw – csk – brass | 0.50 |
|  |  |  |  |
|  | **1/8” W NUTS** |  |  |
| 1685 | 1/8 | Nut – steel - zinc plated | 0.30 |
| 1604 | 1/8 | Nut - brass | 0.30 |
| 1674 | 1/8 | Nut - stainless | 0.30 |
|  |  |  |  |
|  | **5/32” WHIT** |  |  |
|  |  |  |  |
|  |  |  |  |
| 1666 | 5/32 x ¼ | Screw – roundhead-stainless-slotted | 0.50 |
| 0786 | 5/32 x 5/8 | Screw – raised csk – slotted – nickel plated | 0.50 |
| 1863 | 5/32 x ½ | Screw – csk – slot - unplated | 0.50 |
| 1859 | 5/32 x ¾ | Screw – roundhead – steel – slot - unpt | 0.50 |
| 1849 | 5/32 x 1 | Screw – csk – slot - unplated | 0.50 |
| 1850 | 5/32 x 1 | Screw – roundhead – slot - unplated | 0.50 |
| 1128 | 5/32 x 1 ¼ | Screw – roundhead – brass | 0.50 |
| 1148 | 5/32 x 1 ½ | Screw – csk – unplated | 0.50 |
| 1853 | 5/32 x 11/2 | Screw – csk – slot - zinc plated | 0.50 |
| 1854 | 5/32 x 1 ½ | Screw – roundhead – slot - zinc plated | 0.50 |
| 1146 | 5/32 x 2 | Screw – csk | 0.50 |
| 1145 | 5/32 x 2 | Screw – roundhead – zinc plated | 0.50 |
| 1848 | 5/32 x 2 | Screw – roundhead – slot - unplated | 0.60 |
| 1856 | 5/32 x 2 | Screw – roundhead – brass - slot | 1.00 |
|  | **5/32” W NUTS** |  |  |
| 1857 | 5/32 | Nut – steel – zinc plated | 0.50 |
| 1858 | 5/32 | Nut – locknut – steel – zinc plated | 0.50 |
| 0501 | 5/32 | Nut – brass | 0.50 |
| 1629 | 5/32 | Nut – dome –steel - chrome | 0.50 |
| 1795 | 5/32 | Nut – nylock - zinc plated | 0.50 |
| 1855 | 5/32 | Wingnut – zinc plated | 0.50 |
| 1896 | 5/32 | Nut - stainless | 0.50 |
|  |  |  |  |
|  |  |  |  |
|  | **3/16” WHIT** |  |  |
|  |  |  |  |
| 1806 | 3/16 x 3/8 | Screw – csk - slotted | 0.50 |
| 1805 | 3/16 x 3/8 | Screw – raised csk – stainless - slotted | 0.60 |
| 1900 | 3/16 X 3/8 | Screw – csk – Phillips - stainless | 0.50 |
| 1681 | 3/16 x 1/2 | Screw – mush-h – slot – zinc plated | 0.30 |
| 1808 | 3/16 x 1/2 | Screw – csk - slotted | 0.50 |
| 1952 | 3/16 x 1/2 | Screw – csk – slot - stainless | 0.50 |
| 1810 | 3/16 x 1/2 | Screw – roundhead - slotted | 0.50 |
| 0354 | 3/16 x 5/8 | Screw – cheesehead - fully threaded | 0.30 |
| 1451 | 3/16 x 5/8 | Screw – csk – brass – slotted | 0.50 |
| 1967 | 3/16 x 5/8 | Bolt – fully threaded - stainless | 1.00 |
| 1528 | 3/16 x 3/4 | Screw – csk – slotted – unplated | 0.30 |
| 1804 | 3/16 X 3/4 | Screw – mushroom head – slot – zinc | 0.50 |
| 1807 | 3/16 x 1 | Screw – mushroom head – slot – zinc | 0.50 |
| 1156 | 3/16 x 7/8 | Screw – slotted – raised csk – cad plated | 0.30 |
| 0823 | 3/16 x 1 | Screw – csk – slotted – zinc plated | 0.30 |
| 1809 | 3/16 x 1 | Screw – roundhead – brass - slotted | 1.00 |
| 1831 | 3/16 x 1 | Screw – roundhead – steel – slot - unpl | 0.50 |
| 1832 | 3/16 x 1 | Screw – csk – slot - unplated | 0.50 |
| 1147 | 3/16 x 1 ¼ | Screw – csk | 0.50 |
| 1138 | 3/16 x 1 ½ | Screw – csk – slot - zinc plated | 0.50 |
| 1812 | 3/16 x 1 ½ | Screw – csk – slot - unplated | 0.50 |
| 1144 | 3/16 x 1 ½ | Screw – roundhead – zinc plated | 0.50 |
| 1784 | 3/16 x 1 ½ | Screw – roundhead – brass - slotted | 0.60 |
| 1811 | 3/16 x 1 ½ | Screw – roundhead – slot - unplated | 0.50 |
| 1813 | 3/16 x 1 ½ | Screw – mush-head – slot – zinc plated | 0.50 |
| 1815 | 3/16 x 1 ½ | Screw – roundhead – Phillips - zinc plated | 0.50 |
| 1109 | 3/16 x 1 ¾ | Screw – roundhead – slotted | 0.30 |
| 0671 | 3/16 x 2 | Bolt | 0.50 |
| 1139 | 3/16 x 2 | Screw – csk – zinc plated | 0.30 |
| 1107 | 3/16 x 2 | Screw – roundhead – slotted - unplated | 0.30 |
| 1140 | 3/16 x 2 | Screw – roundhead – slotted – zinc plated | 0.30 |
| 1816 | 3/16 x 2 | Screw – roundhead – Phillips – zinc plated | 0.50 |
| 1814 | 3/16 x 2 | Screw – csk – Phillips – zinc plated | 0.50 |
| 1819 | 3/16 x 2 | Screw – mushhead – slot - zinc plated | 0.50 |
| 1820 | 3/16 x 2 | Screw – csk – slot - unplated | 0.50 |
| 1108 | 3/16 x 2 ½ | Screw – csk – slotted | 0.30 |
| 1141 | 3/16 x 2 ½ | Screw – roundhead – zinc plated | 0.30 |
| 1821 | 3/16 x 2 ½ | Screw – mush-head – slot - zinc plated | 0.50 |
| 1142 | 3/16 x 3 | Screw – csk – zinc plated | 0.30 |
| 1817 | 3/16 x 3 | Screw – roundhead – slot - unplated | 0.50 |
| 1818 | 3/16 x 3 | Screw – mush-head – slot - zinc plated | 0.50 |
|  |  |  |  |
|  | **3/16” W NUTS** |  |  |
| 1682 | 3/16 | Nut – locknut - zinc plated | 0.30 |
| 1780 | 3/16 | Nut – plain hex - zinc plated | 0.50 |
| 1250 | 3/16 | Nut – brass - unplated | 0.50 |
| 1181 | 3/16 | Nut – brass | 0.50 |
| 1247 | 3/16 | Nut – dome - chrome | 0.70 |
| 1683 | 3/16 | Nut – wingnut – steel - | 1.00 |
| 1897 | 3/16 | Nut - stainless | 0.50 |
|  |  |  |  |
|  |  |  |  |
|  | **¼” WHIT** |  |  |
| 0907 | ¼ x 3/8 | Setscrew – cad plated | 0.30 |
| 0924 | ¼ x 3/8 | Screw – csk - slotted – stainless | 1.00 |
| 1239 | ¼ x 3/8 | Screw - cheesehead | 1.00 |
| 1510 | ¼ x 3/8 | Grubscrew – Allen socket head | 0.50 |
| 0908 | ¼ x ½ | Setscrew – cad plated | 0.30 |
| 1137 | ¼ x ½ | Screw – roundhead - unplated | 0.30 |
| 0812 | ¼ x ½ | Screw – roundhead – with nut – stainless | 1.00 |
| 1341 | ¼ x ½ | Screw – mush – slotted - zinc plated | 0.30 |
| 1632 | ¼ x ½ | Screw – mush – slotted - unplated | 0.30 |
| 1606 | ¼ x ½ | Screw – raised csk – slotted – head 11.4 mm | 0.50 |
| 1607 | ¼ x ½ | Screw – raised csk – slotted – head 12.6 mm | 0.60 |
| 2005 | ¼ X 5/8 | Screw – mush – slotted - zinc plated | 0.60 |
| 0956 | ¼ x ¾ | Bolt | 0.50 |
| 0906 | ¼ x ¾ | Setscrew – cad plated | 0.50 |
| 1245 | ¼ x ¾ | Screw – csk – slotted - unplated | 0.50 |
| 1136 | ¼ x ¾ | Screw – roundhead – steel - unplated | 0.30 |
| 1423 | ¼ x ¾ | Screw – mush – slotted - zinc plated | 0.50 |
| 1835 | ¼ x ¾ | Screw – mush-head – Phillips - zinc | 0.50 |
| 0529 | ¼ x 7/8 | Screw – domed cheesehead – nickel plated | 1.50 |
| 0903 | ¼ x 1 | Bolt and nut | 0.50 |
| 0729 | ¼ x 1 | Setscrew | 0.50 |
| 0694 | ¼ x 1 | Setscrew – unplated | 0.50 |
| 0905 | ¼ x 1 | Setscrew - cad plated | 0.50 |
| 0854 | ¼ x 1 | Screw – csk – slotted – zinc plated | 0.30 |
| 1824 | ¼ x 1 | Screw – csk – slot - unplated | 0.50 |
| 0355 | ¼ x 1 | Screw – csk – raised head – mild steel | 0.30 |
| 0782 | ¼ x 1 | Screw – csk – raised head – stainless | 0.60 |
| 1135 | ¼ x 1 | Screw – roundhead – zinc plated | 0.30 |
| 1822 | ¼ x 1 | Screw – roundhead – slot - unplated | 0.50 |
| 1523 | ¼ x 1 | Screw – roundhead - brass slotted | 1.00 |
| 1424 | ¼ x 1 | Screw – mush – slotted - zinc plated | 0.50 |
| 1833 | ¼ x 1 | Screw – mush-head – Phillips – zinc plated | 0.50 |
| 1834 | ¼ x 1 | Screw – roundhead – Phillips - zinc plated | 0.50 |
|  |  |  |  |
| 0448 | ¼ x 1 3/16 | Stud | 0.50 |
| 0904 | ¼ x 1 ¼ | Bolt and nut | 0.30 |
| 0909 | ¼ x 1 ½ | Bolt and nut | 0.30 |
| 1132 | ¼ x 1 ½ | Screw – csk –slotted - zinc plated | 0.30 |
| 1425 | ¼ x 1½ | Screw – mush – slotted - zinc plated | 0.50 |
| 1823 | ¼ x 1 ½ | Screw – roundhead – slot - unplated | 0.50 |
| 1825 | ¼ x 1 ½ | Screw – roundhead – slot - zinc plated | 0.50 |
| 0911 | ¼ x 2 | Bolt and nut – TL 5/8” | 0.30 |
| 1130 | ¼ x 2 | Screw – csk – slotted – nickel plated | 0.30 |
| 1134 | ¼ x 2 | Screw – roundhead – zinc plated | 0.50 |
| 1426 | ¼ x 2 | Screw – mush – slotted - zinc plated | 0.60 |
| 1827 | ¼ x 2 | Screw – csk – slotted - unplated | 0.60 |
| 1828 | ¼ x 2 | Screw – roundhead – slot - brass | 1.50 |
| 0912 | ¼ x 2 ½ | Bolt and nut – TL 5/8” | 0.30 |
| 0449 | ¼ x 2 ½ | Stud | 0.60 |
| 1133 | ¼ x 2 ½ | Screw – roundhead | 0.50 |
| 1427 | ¼ x 2½ | Screw – mush – slotted - zinc plated | 1.00 |
|  |  |  |  |
| 1129 | ¼ x 3 | Screw – csk – slotted | 0.50 |
| 1131 | ¼ x 3 | Screw – csk – slotted – nickel plated | 0.50 |
| 1829 | ¼ x 3 | Screw – csk – slot - zinc plated | 0.50 |
| 1158 | ¼ x 3 | Screw – roundhead – slotted | 0.50 |
| 1573 | ¼ x 3 | Screw – mush – slotted - zinc plated | 1.00 |
| 1829 | ¼ x 3 | Screw – csk – slot - |  |
|  | **¼” WHIT NUTS** |  |  |
| 1830 | ¼ | Nut – hex - zinc plated | 0.30 |
| 0910 | ¼ | Nut – cad plated – 11.2 mm head | 0.30 |
| 1248 | ¼ | Nut – dome – chrome | 1.00 |
| 1593 | ¼ | Nut – dome - stainless | 1.00 |
| 1522 | ¼ | Nut - brass | 0.50 |
| 1672 | ¼ | Nut – square - zinc plated | 0.30 |
| 1775 | ¼ | Nut – hex - stainless | 0.50 |
|  |  |  |  |
|  | **5/16” WHIT** |  |  |
| 0357 | 5/16 X 5/16 | Screw – Roundhead - zinc plated | 0.30 |
| 0484 | 5/16 x ½ | Bolt – zinc plated and nut | 0.30 |
| 0555 | 5/16 x ½ | Capscrew – socket head | 0.50 |
| 1631 | 5/16 x 9/16 | Screw – slotted mush head - zinc plated | 0.50 |
| 0554 | 5/16 x 5/8 | Capscrew – socket head | 0.50 |
| 1168 | 5/16 x 5/8 | Screw – csk – slotted – stainless | 1.00 |
| 1546 | 5/16 x 5/8 | Screw – csk – slotted - zinc plated | 0.50 |
| 1081 | 5/16 x ¾ | Screw – raised csk – slotted – chromed | 1.50 |
| 1769 | 5/16 X ¾ | Screw – csk – slotted – zinc - seconds | 0.50 |
| 1167 | 5/16 x 7/8 | Screw – roundhead – slotted – stainless | 0.50 |
| 0816 | 5/16 x 7/8 | Screw – cheesehead | 0.30 |
| 1380 | 5/16 x 1 | Screw – csk – slotted - brass | 1.00 |
| 1513 | 5/16 X 1 | Screw – cheesehead – slotted - unplated | 1.00 |
| 0553 | 5/16 x 1 ¼ | Capscrew – socket head | 0.60 |
| 0563 | 5/16 x 1 ¼ | Coachbolt - black | 0.60 |
| 1246 | 5/16 x 1 ¼ | Screw - csk - slotted – fully threaded | 0.50 |
| 0424 | 5/16 x 1 ½ | Bolt – TL 5/8” - unplated | 0.50 |
| 0425 | 5/16 x 1 ¾ | Bolt – TL ¾” - unplated | 0.50 |
| 0573 | 5/16 x 2 | Bolt – TL ¾’’ – and nut | 0.50 |
| 0556 | 5/16 x 2 ¾ | Capscrew – socket head | 2.00 |
| 0800 | 5/16 x 3 | Bolt – TL 1” – and nut | 0.60 |
| 0356 | 5/16 x 3 ¼ | Capscrew – socket head | 2.50 |
| 0858 | 5/16 | Allthread | 0.30 p inch |
|  | **5/16” W NUTS** |  |  |
| 0415 | 5/16 | Nut – plain hex – 13 mm head | 0.30 |
| 1860 | 5/16 | Nut – plain hex - unplated | 0.30 |
| 0498 | 5/16 | Nut – dome / acorn – brass – nickel plated | 2.00 |
| 1249 | 5/16 | Nut – dome - chrome | 2.00 |
| 0502 | 5/16 | Nut – nylock | 0.60 |
| 0929 | 5/16 | Nut – split thread lock (Aerotight) | 0.50 |
| 0932 | 5/16 | Wingnut – unplated | 0.50 |
| 0933 | 5/16 | Wingnut – zinc plated | 0.50 |
| 1898 | 5/16 | Nut - stainless | 0.60 |
|  |  |  |  |
|  | **3/8” WHIT** |  |  |
|  |  |  |  |
| 0991 | 3/8 x ½ | Screw – csk slotted – black | 0.50 |
| 0645 | 3/8 x ¾ | Screw – csk – slotted | 0.30 |
| 0571 | 3/8 x 1 | Setscrew – cad plated | 0.50 |
| 1836 | 3/8 x 1 | Setscrew - unplated | 0.60 |
| 1097 | 3/8 x 1 ¼ | Bolt – TL ¾ “ | 0.50 |
| 0421 | 3/8 x 1 ½ | Bolt | 0.50 |
| 0587 | 3/8 x 1 ¾ | Capscrew – socket head, HT,  TL 1 1/8 | 0.50 |
| 0576 | 3/8 x 2 | Bolt – TL 7/8’’ | 0.50 |
| 0574 | 3/8 x 2 | Bolt –TL 1’’ – zinc plated | 0.50 |
| 0575 | 3/8 x 2 | Bolt –TL1 ½ ’’ – zinc plated | 0.50 |
| 1649 | 3/8 x 2 | Screw - roundhead unplated - seconds | 0.50 |
| 0508 | 3/8 x 3 | Bolt – drilled – cad plated – TL ½” | 0.50 |
| 1838 | 3/8 x 3 ½ | Bolt - TL ¾ “ - ¼” deep head- unplatd | 0.60 |
| 1840 | 3/8 x 3 ½ | Bolt – TL 1” – 5/16 deep head - unplated | 0.60 |
| 1837 | 3/8 x 4 | Bolt – TL 1” - unplated | 2.00 |
| 0557 | 3/8 x 4 | Capscrew – socket head | 2.80 |
| 0435 | 3/8 x 7 | Bolt | 2.00 |
|  | **3/8” W NUTS** |  |  |
| 0358 | 3/8 | Nut – plain hex – 15 mm A/F | 0.50 |
| 1839 | 3/8 | Nut – plain hex – 18 mm A/F | 0.60 |
| 0499 | 3/8 | Nut – dome / acorn – brass – nickel plated – 14.7 mm deep | 3.00 |
| 1627 | 3/8 | Nut – dome / acorn – brass – chrome plated – 13.4 mm deep | 3.00 |
| 0503 | 3/8 | Nut – nylock | 1.00 |
| 1506 | 3/8 | Wingnut - zinc plated | 1.00 |
| 1899 | 3/8 | Nut - stainless | 1.00 |
|  |  |  |  |
|  | **7/16” WHIT** |  |  |
| 1785 | 7/16 x 1 | Setscrew | 1.00 |
| 0584 | 7/16 x 1 ½ | Bolt – HT | 1.00 |
| 0530 | 7/16 x 1 ¾ | Screw – cheesehead | 0.50 |
| 0949 | 7/16 x 2 | Bolt – TL 1” - unplated | 0.60 |
| 0946 | 7/16 x 2 | Bolt – TL 1 ¼” – zinc plated | 1.00 |
| 1862 | 7/16 x 2 ¼ | Bolt – TL 1” - unplated | 1.00 |
| 1842 | 7/16 x 2 ½ | Bolt – TL 1” - unplated | 1.00 |
| 0895 | 7/16 x 3 | Bolt – TL 1” – 18 mm head | 1.50 |
| 0794 | 7/16 x 4 | Bolt – TL 1” – 18 mm head | 2.00 |
|  | **7/16” W NUTS** |  |  |
| 0860 | 7/16 | Nut – plain hex – 18 mm head | 0.30 |
| 0469 | 7/16 | Nut – dome / acorn – brass – nickel plated | 3.50 |
|  |  |  |  |
|  | **½” WHIT** |  |  |
| 0913 | ½ x ¾ | Setscrew | 0.50 |
| 0558 | ½ x 7/8 | Capscrew – socket head | 1.00 |
| 0914 | ½ x 1 | Setscrew | 0.50 |
| 0915 | ½ x 1 ¼ | Bolt and nut | 0.50 |
| 0566 | ½ x 1 ½ | Bolt - TL 1”– and nut - unplated | 1.50 |
| 0683 | ½ x 1 ½ | Screw – csk – socket head – stainless – with nuts (extra nuts) | 1.00 |
| 0916 | ½ x 1 ¾ | Setscrew | 1.00 |
| 1864 | ½ x 1 ¾ | Bolt – with nut - unplated | 1.00 |
| 0730 | ½ x 2 | Setscrew - unplated | 1.00 |
| 1888 | ½ X 2 | Setscrew – square head | 1.00 |
| 1865 | ½ x 2 | Bolt- TL 1 ¼” - galv | 1.00 |
| 1866 | ½ x 2 | Bolt – TL 1” - unplated | 1.00 |
| 0957 | ½ x 2 ½ | Bolt – T/L/ 1 ¼” – and nut | 0.50 |
| 0646 | ½ x 2 ½ | Setscrew - unplated | 0.50 |
|  |  |  |  |
| 1623 | ½ X 2 | Screw – roundhead- slotted - brass | 2.00 |
| 0917 | ½ x 3 | Bolt and nut – TL 1” | 0.60 |
| 1867 | ½ x 3 | Bolt – TL 1 ½ - stainless | 4.00 |
| 0943 | ½ x 3 ½ | Bolt – TL 1” – with nut - unplated | 0.60 |
| 0669 | ½ x 3 ½ | Bolt & nut – zinc plated | 1.00 |
| 0850 | ½ x 4 | Bolt and nut | 1.00 |
| 1861 | ½ x 5 ½ | Bolt – TL 1” - galv | 2.00 |
|  | **½” WHIT NUTS** |  |  |
| 0568 | ½ | Nut – 10.6 mm deep – unplated | 0.60 |
| 1634 | ½ | Nut – 11.05 deep - unplated | 0.60 |
| 1868 | ½ | Nut – 23.5mm wide - seconds | 1.00 |
| 1296 | ½ | Nylock nut – zinc-chromate plated | 2.00 |
| 0964 | ½ | Wingnut | 2.00 |
| 1557 | ½ | Nut - brass | 2.00 |
| 1630 | ½ | Nut – dome – brass - chromed | 2.00 |
| 1984 | ½ | Nut - stainless | 2.00 |
|  |  |  |  |
|  |  |  |  |
|  | **9/16” WHIT** |  |  |
| 1635 | 9/16 | Nut – hex - unplated | 1.00 |
|  |  |  |  |
|  | **5/8” WHIT** |  |  |
| 0359 | 5/8 x 1 | Bolt – square head - cup point | 1.00 |
| 1242 | 5/8 x 1 | Bolt – square head – flat point | 1.00 |
| 0564 | 5/8 x 1 ¼ | Setscrew and nut | 2.00 |
| 0360 | 5/8 x 1 ½ | Bolt – square head - cup point | 1.00 |
| 0897 | 5/8 x 1 ¾ | Bolt – TL 1 ¼ - with nut - unplated | 1.00 |
| 1241 | 5/8 x 1 7/8 | Capscrew – fully threaded | 1.00 |
| 0647 | 5/8 x 2 | Bolt – zinc plated | 0.30 |
| 1243 | 5/8 x 2 | Bolt – square head – flat point | 2.00 |
| 1587 | 5/8 x 2 | Stud – brass – with shoulder | 5.00 |
| 0426 | 5/8 x 2 ½ | Bolt – zinc plated | 1.00 |
| 0877 | 5/8 x 2 ½ | Bolt - TL 1 ½” – and nut | 0.60 |
| 1873 | 5/8 X 2 ½” | Bolt – TL 1” – and nut | 2.00 |
| 0921 | 5/8 x 2 ½ | Bolt – stainless | 4.00 |
| 0852 | 5/8 x 3 | Bolt and nut – unplated | 1.50 |
| 0879 | 5/8 x 3 | Bolt and nut – zinc plated | 2.00 |
| 0427 | 5/8 x 3 ½ | Bolt – zinc plated | 2.00 |
| 1870 | 5/8 x 3 ½ | Setscrew - galv | 2.00 |
| 1869 | 5/8 x 4 | Bolt - galv | 2.00 |
| 0428 | 5/8 x 4 ½ | Bolt – zinc plated | 3.00 |
| 1871 | 5/8 x 4 ½ | Bolt - galv | 2.00 |
| 1872 | 5/8 x 5 | Bolt - galv | 3.00 |
|  | **5/8” WHIT NUTS** |  |  |
| 0922 | 5/8 | Nut – unplated | 0.50 |
| 0438 | 5/8 | Nut – zinc plated | 0.50 |
| 0628 | 5/8 | Nut – nylock – zinc plated | 1.00 |
| 1636 | 5/8 | Nut – nylock - zincchromate | 1.50 |
|  |  |  |  |
|  | **¾” WHIT** |  |  |
|  |  |  |  |
| 1875 | ¾ x 1 ¼ | Bolt - unplated | 1.00 |
| 1874 | ¾ x 2 | Bolt – TL 1 ½ - unplated | 1.00 |
| 1876 | ¾ x 2 | Setscrew - unplated | 1.50 |
| 0567 | ¾ x 2 ½ | Bolt –TL 1 ¾” – and nut | 1.00 |
| 0559 | ¾ x 2 ¾ | Capscrew - socket head, black, TL 2” | 2.00 |
| 0862 | ¾ x 3 | Bolt and nut – zinc plated | 5.00 |
| 0827 | ¾ x 6 | Bolt and nut | 4.00 |
| 0513 | ¾ x 12 | Bolt – TL 2 ¼ - and nut | 6.00 |
|  | **¾” WHIT NUTS** |  |  |
| 0439 | ¾ | Nut – zinc plated | 0.70 |
| 0936 | ¾ | Nut – nylock | 1.00 |
|  |  |  |  |
|  | **7/8” WHIT** |  |  |
|  |  |  |  |
| 1877 | 7/8 x 3 | Bolt – TL 2” - unplated | 4.00 |
| 1878 | 7/8 x 3 ¼ | Bolt – TL 1 ¾” - unplated | 4.00 |
|  | **7/8 “WHIT NUTS** |  |  |
| 0423 | 7/8 | Nut – plain hex - unplated | 1.00 |
|  |  |  |  |
| 1880 | 7/8 | Nut – Aerotite split-thread locknut | 2.00 |
|  |  |  |  |
|  | 1” WHIT |  |  |
|  |  |  |  |
| 1883 | 1 x 3 ½ | Setscrew - unplated | 5.00 |
| 0422 | 1 x 6 | Bolt and nut | 7.00 |
|  | **1” WHIT NUTS** |  |  |
| 0769 | 1” | Nut – plain hex | 5.00 |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  | **1 ¼” WHIT** |  |  |
| 0728 | 1 ¼” | Nut – plain hex | 3.00 |
| 1879 | 1 ¼ | Nut - slotted | 5.00 |

**U.N.F. (Unified National Fine)**

**(Pitch angle 60 degrees)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Code** | **Diameter & Length** | **Item** | **Price** |
|  | **6/40 UNF** |  |  |
| 1619 | 6/40 X 1 ¾ | Screw – roundhead – fully threaded – cad plated | 1.50 |
| 1906 | 6/40 | Nut - stainless | 1.50 |
|  |  |  |  |
|  |  |  |  |
|  | **10/32 UNF** |  |  |
| 0864 | “10/32” (10G x 32tpi) x 3/8 | Screw – csk – with fitted washer – Phillips – zinc plated | 0.20 |
| 1602 | “10/32” (10G x 32tpi) x 1/2 | Screw – panhead – slotted – z/plated | 0.50 |
| 0585 | “10/32” (10G x 32tpi) x 7/16 | Screw – csk – Phillipshead –zinc chromate plated | 0.50 |
| 0361 | “10/32” (10G x 32tpi) x ½ | Setscrew – hex head | 0.50 |
| 0588 | “10/32” (10G x 32tpi) x 5/8 | Bolt – TL 3/8” - grey | 0.50 |
| 0960 | “10/32” (10G x 32tpi) x 5/8 | Bolt – TL 3/8” – silver | 1.00 |
| 1739 | “10/32” (10G x 32tpi) x 5/8 | Screw – roundhead – Phillips – TL ¼” | 0.50 |
| 1001 | “10/32” (10G x 32tpi) x 5/8 | Screw – panhead – slotted – stainless | 0.90 |
| 0869 | “10/32” (10G x 32tpi) x ¾ | Bolt – TL 3/8” | 1.00 |
| 0962 | “10/32” (10G x 32tpi) x ¾ | Screw – raised csk – stainless | 1.00 |
| 0215 | “10/32” (10g x 32tpi) x 1 | Screw – mushhead – slotted – cad – head 10.35 mm | 1.00 |
| 0362 | “10/32” (10G x 32tpi) x 1 | Bolt – zinc plated – TL 7/8 | 0.50 |
| 0727 | “10/32” (10G x 32tpi) x 1 | Screw – raised csk – stainless | 1.50 |
| 0902 | “10/32” (10G x 32tpi) x 1 5/8 | Bolt – zinc-chromate – TL 3/8” | 0.50 |
| 0919 | “10/32” (10G x 32tpi) x 2 ¾ | Bolt – cad plated – TL ½” | 0.50 |
| 0461 | “10/32” (10G x 32tpi) x 4 | Bolt – drilled – cad plated  – TL 3/8” | 1.00 |
| 0363 | “10/32” (10G x 32tpi) x 6 | Bolt – cad plated | 1.00 |
|  | **UNF 10/32 NUTS** |  |  |
| 0974 | “10/32” (10G x 32tpi) | Nut – plain hex | 0.50 |
| 0364 | “10/32” (10G x 32tpi) | Nut – brass | 0.50 |
| 0511 | “10/32” (10G x 32tpi) | Nut – slotted | 0.80 |
| 0975 | “10/32” (10G x 32tpi) | Locknut | 0.80 |
| 1797 | “10/32” (10G x 32tpi) | Nut - nylock | 1.00 |
|  |  |  |  |
|  | **¼” UNF** |  |  |
| 0416 | ¼ x 3/8 | Screw – panhead – Phillips | 0.50 |
| 0455 | ¼ x 3/8 | Screw – cheesehead | 0.50 |
| 0959 | ¼ x ½ | Setscrew – mild - unplated | 0.50 |
| 0958 | ¼ x ½ | Setscrew – HT (Grade 5) - black | 0.80 |
| 1970 | ¼ x ½ | Setscrew – HT – zinc-chromate plated | 1.20 |
| 0590 | ¼ x 5/8 | Bolt – 12 point drive (UNJF - Titanium) | 1.00 |
| 1971 | ¼ x 3/4 | Bolt – HT – TL 3/8” – zinc-chromate | 1.30 |
| 1058 | ¼ x 7/8 | Screw – csk – slotted – zincpl | 1.00 |
| 1594 | ¼ x 1 | Screw - cheesehead | 1.00 |
|  |  |  |  |
| 0950 | ¼ x 1 ¼ | Bolt – TL ¾” | 1.00 |
| 0951 | ¼ x 1 ¼ | Bolt – TL ¾” – HT (Grade 5) | 1.50 |
| 0942 | ¼ x 2 | Bolt – HT (Grade 5) – TL3/4” | 1.50 |
| 0861 | ¼ x 2 3/8 | Bolt – TL 3/8” – zincchromate pl | 1.30 |
| 1588 | ¼ x 1 | Bolt – cad – ½” TL | 1.00 |
| 0896 | ¼ x 2 ½ | Bolt – HT (Grade 5) | 1.60 |
| 0952 | ¼ x 2 ½ | Bolt – T/L/ ¾ - HT (Gr5)- zincpl | 1.60 |
| 0446 | ¼ x 2 ¾ | Bolt – drilled – cad plated | 1.50 |
|  |  |  |  |
|  | **¼” UNF NUTS** |  |  |
| 1783 | ¼ | Nut – plain hex – s/soiled | 0.50 |
| 0510 | ¼ | Nut – castle – cad plated | 0.50 |
| 1796 | ¼ | Nut – castle - unplatd | 0.50 |
| 0866 | ¼ | Nut – self-locking – zincchromate – L-19 type | 0.50 |
| 1609 | ¼ | Nut – nylock - zincchromate | 1.00 |
|  |  |  |  |
|  |  |  |  |
|  | **5/16” UNF** |  |  |
|  |  |  |  |
| 0417 | 5/16 x ½ | Setscrew - black | 0.80 |
| 1972 | 5/16 X ¾ | Bolt – HT – TL 1/2” – zinc-chromate | 1.50 |
| 0953 | 5/16 x 1 | Setscrew – mild - unplated | 0.80 |
| 0940 | 5/16 x 1 | Setscrew – HT (Grade 5) | 1.50 |
|  |  |  |  |
| 0579 | 5/16 x 1 ¼ | Bolt- TL ½ “-pascad-drilled head | 0.50 |
| 0882 | 5/16 x 1 ¼ | Bolt – HT (Grade 5) –  TL 7/8” | 0.80 |
| 0892 | 5/16 x 1 ½ | Bolt – HT (Grade 5) | 1.00 |
| 1658 | 5/16 x 1 ½ | Bolt – shoulder – thread 5/16 – shaft 3/8 x 7/8 | 2.00 |
| 0938 | 5/16 x 2 | Bolt – HT (Grade 5) – TL1” | 0.50 |
| 0971 | 5/16 x 4 | Bolt – TL ½’ – drilled – zinc plated | 2.00 |
|  | **5/16” UNF NUTS** |  |  |
| 0788 | 5/16 | Nut – plain hex | 0.50 |
| 0582 | 5/16 | Nut – self-locking with flange – K-nuts | 0.50 |
| 0586 | 5/16 | Nut –slotted locknut –cad pl | 0.50 |
| 0873 | 5/16 | Nut – nylock | 1.50 |
| 0460 | 5/16 | Nut – brass – deep – manifold | 3.00 |
|  |  |  |  |
|  | **3/8” UNF** |  |  |
| 1735 | 3/8 x ½ | Setscrew - Gr 8 - zinc plated | 1.00 |
| 1736 | 3/8 x ¾ | Setscrew – Gr 8 - zinc plated | 1.00 |
| 1637 | 3/8 x 3/4 | Coachbolt – square under head – domed head | 2.00 |
| 1973 | 3/8 x 1 | Bolt – HT – TL 1/2” – zinc-chromate | 2.20 |
| 0572 | 3/8 x 1 3/16 | Bolt –TL 9/16’’ – pascad | 0.60 |
| 0429 | 3/8 x 1 3/16 | Bolt – TL 7/8’’ – unpl | 0.60 |
| 1302 | 3/8 x 1 ¼ | Setscrew – mild - unplated | 0.50 |
| 0970 | 3/8 x 1 3/8 | Bolt – socket head – TL 5/8” | 0.50 |
| 0899 | 3/8 x 1 ½ | Bolt – HT (Grade 5) - TL 1” - black | 2.00 |
| 1999 | 3/8 X 1 9/16 | Stud – TL ½” and ½” | 6.00 |
| 0430 | 3/8 x 1 5/8 | Bolt – drilled – TL 5/8” - cadpl | 1.50 |
| 0457 | 3/8 x 1 5/8 | Stud –TL ½” + ¾” | 1.60 |
| 1650 | 3/8 x 1 7/8 | Bolt – black - seconds | 1.00 |
| 0569 | 3/8 x 2 3/16 | Bolt –TL 5/8” - pascadpl | 1.80 |
| 0900 | 3/8 x 2 ½ | Bolt – HT (Grade 5) | 2.00 |
| 0450 | 3/8 x 2 5/8 | Bolt | 1.00 |
| 1656 | 3/8 x 2 ¾ | Bolt – TL 7/8” - seconds | 0.50 |
| 0968 | 3/8 x 3 | Bolt – TL ½’ – drilled | 2.40 |
| 0898 | 3/8 x 3 ½ | Bolt – mild – TL 1” | 2.00 |
| 0894 | 3/8 x 4 | Bolt – mild – TL 1” | 2.00 |
| 0881 | 3/8 x 4 | Bolt – HT (Grade 5) – TL 1” | 3.00 |
|  | **3/8 “ UNF NUTS** |  |  |
| 0478 | 3/8 | Nut – plain hex – zinc plated | 0.80 |
| 0463 | 3/8 | Nut – cad plated | 0.80 |
| 0570 | 3/8 | Nut – slotted – cad plated | 0.80 |
| 1948 | 3/8 | Nut – castle – cad plated | 1.00 |
| 1293 | 3/8 | Nut – dome - chromed | 7.50 |
| 0870 | 3/8 | Nut – nylock | 1.00 |
| 1532 | 3/8 | Nut – castle - unplated | 1.00 |
|  |  |  |  |
|  | **7/16” UNF** |  |  |
| 0432 | 7/16 x 7/8 | Bolt – drilled – cad plated | 1.00 |
| 0954 | 7/16 x 1 | Setscrew – mild | 0.50 |
| 1094 | 7/16 x 1 | Setscrew – HT (Grade 5) | 1.00 |
| 0872 | 7/16 x 1 ¼ | Setscrew | 1.00 |
| 1651 | 7/16 x 1 3/8 | Screw – slot panhead – TL ¾” – with castle nut | 1.00 |
| 0939 | 7/16 x 1 ½ | Bolt – HT (Grade 5) – TL 1 ¼ | 1.00 |
| 0447 | 7/16 x 1 7/8 | Bolt – drilled – cad plated | 1.00 |
| 0944 | 7/16 x 2 | Bolt - HT (Grade 5) – TL 1” | 1.50 |
| 0945 | 7/16 x 2 ¼ | Bolt – HT (Grade 5) – TL1¼ - zinc plated | 1.50 |
| 1654 | 7/16 x 2 ½ | Bolt – TL 1” - seconds | 1.00 |
| 1647 | 7/16 x 3 | Bolt and nut - seconds | 1.00 |
| 0937 | 7/16 x 3 ½ | Bolt HT (Grade 5) – TL 1 ¼” | 1.50 |
| 0797 | 7/16 x 4 | Bolt – TL 1” – unplated | 2.00 |
| 0947 | 7/16 x 4 | Bolt – HT (Grade 5) – TL 1” | 2.50 |
|  | **7/16” UNF NUTS** |  |  |
| 0473 | 7/16 | Nut – deep – cad plated | 0.60 |
| 0477 | 7/16 | Nut – slotted | 0.60 |
| 0476 | 7/16 | Nut – castle | 1.00 |
| 0470 | 7/16 | Nut – nylock | 1.00 |
|  |  |  |  |
|  | **½” UNF** |  |  |
| 0955 | ½ x 1 | Setscrew | 1.00 |
| 0941 | ½ x 1 | Setscrew – HT (Grade 5) | 1.50 |
| 0948 | ½ x 1 ½ | Bolt – TL 1 ¼” – HT (Grade 5) | 1.50 |
| 0901 | ½ x 1 ½ | Setscrew – HT (Grade 8) | 2.00 |
| 0462 | ½ x 2 | Bolt – cad plated | 2.50 |
| 0418 | ½ x 2 | Stud –TL ½” + 1 1/8” | 2.50 |
| 0935 | ½ x 2 ½ | Bolt – TL 1 ½” | 2.00 |
| 0419 | ½ x 2 ½ | Bolt – drilled | 2.00 |
| 0565 | ½ x 3 | Bolt - mild –TL 1 ¼’’ | 3.00 |
| 0801 | ½ x 3 | Bolt – HT(Grade 8) – TL1 ¼”  And nut | 3.00 |
| 0485 | ½ x 3 ½ | Bolt and nut | 2.50 |
| 1655 | ½ x 5 ½ | Bolt – TL 1 ¼ - seconds | 3.00 |
| 0790 | ½ x 6 | Bolt - mild - TL 1 ½” | 3.00 |
| 0789 | ½ x 6 | Bolt HT (Grade 5) – TL 13/8” | 4.00 |
|  | **½” UNF NUTS** |  |  |
| 1642 | ½ | Nut – stainless – recessed one side | 2.00 |
| 0471 | ½ | Nut – plain hex. deep | 1.50 |
| 1773 | ½ | Nut - HT | 2.00 |
| 0580 | ½ | Nut – slotted locknut – zincchrom | 2.00 |
| 1297 | ½ | Nylock nut - zinc-chromate | 2.00 |
| 1589 | ½ | Nut – brass – 8 mm deep | 3.00 |
| 1730 | ½ | Nut – castle - zinc-chromate | 5.50 |
|  |  |  |  |
|  | **9/16” UNF** |  |  |
| 0433 | 9/16 x 1 ½ | Bolt | 2.00 |
| 0436 | 9/16 x 1 ¾ | Bolt | 2.50 |
| 0437 | 9/16 x 2 | Bolt | 2.50 |
| 0482 | 9/16 x 6 | Bolt | 5.00 |
|  | **9/16” UNF NUTS** |  |  |
| 0434 | 9/16 | Nut | 2.50 |
| 1055 | 9/16 | Nut – slotted | 2.50 |
| 0934 | 9/16 | Nylock nut - zinc-chromate | 2.50 |
| 1782 | 9/16 | Nylock nut – cad plated | 2.50 |
| 1366 | 9/16 | Wheelnut - RHT | 5.00 |
| 1364 | 9/16 | Wheelnut – LHT - cad plated | 7.00 |
|  |  |  |  |
|  | **5/8” UNF** |  |  |
| 0793 | 5/8 x 2 | Bolt – mild – TL 1 5/8 | 2.40 |
| 0792 | 5/8 x 2 | Bolt – HT (Grade 5) TL 1 5/8” | 2.50 |
| 0772 | 5/8 x 2 | Bolt – HT (Grade 8) | 2.00 |
| 0885 | 5/8 x 2 1/8 | Bolt – drilled – TL ½ “ | 2.50 |
| 0431 | 5/8 x 2 5/8 | Bolt | 3.00 |
| 0464 | 5/8 x 3 ¼ | Bolt – drilled – cad plated | 4.00 |
| 0475 | 5/8 x 3 ½ | Bolt – drilled – cad plated | 4.00 |
| 1640 | 5/8 x 3 ½ | Bolt with nut - seconds | 1.00 |
| 0483 | 5/8 x 5 ¾ | Bolt – drilled – cad plated | 4.50 |
|  | **5/8” UNF NUTS** |  |  |
| 0509 | 5/8 | Nut – plain hex | 2.00 |
| 1036 | 5/8 | Nut – zinc plated | 2.50 |
| 0650 | 5/8 | Nut – plain hex – HT | 3.00 |
| 0465 | 5/8 | Nut – slotted | 3.00 |
| 0456 | 5/8 | Nut – castle – cad plated | 5.00 |
| 0678 | 5/8 | Nut – nylock – zinc chromate | 5.00 |
| 1959 | 5/8 | Nut – lock - zincchromate | 7.00 |
| 2006 | 5/8 | Nut – stainless - | 3.50 |
|  |  |  |  |
|  |  |  |  |
|  | **¾” UNF** |  |  |
| 1641 | ¾ x 4 | Bolt – HT with nut -seconds | 2.00 |
|  | **¾ UNF NUTS** |  |  |
| 1653 | ¾ | Nut – plain hex - seconds | 1.50 |
| 1657 | ¾ | Nut – plain hex - LHT | 2.00 |
| 0472 | ¾ | Nut – zinc plated | 2.50 |
| 1365 | ¾ | Nut – slotted - deep | 6.00 |
| 1035 | ¾ | Nut – wheelnut | 5.00 |
| 1645 | ¾ | Nut – castle - seconds | 3.00 |
| 1646 | ¾ | Nut – slotted - seconds | 3.00 |
|  |  |  |  |
|  | **7/8” UNF** |  |  |
| 0497 | 7/8 | Nut – slotted – “Dufor 8” | 4.00 |
| 0973 | 7/8 | Nylock nut | 5.00 |
|  |  |  |  |
|  | **1” UNF** |  |  |
| 1051 | 1 x 2” | Bolt – NOTE ; 14 TPI | 4.00 |
|  |  |  |  |
|  | **1 1/8” UNF** |  |  |
| 0474 | 1 1/8 | Nut – castle | 5.00 |
| 0717 | 1 1/8 | Locknut – slotted | 5.00 |

**U.N.E.F. (Unified National Extra Fine)**

(Pitch angle 60 degrees)

|  |  |  |  |
| --- | --- | --- | --- |
| **Code** | **Diameter & length** | **Item** | **Price** |
|  | 1 “ UNEF |  |  |
|  |  |  |  |
| 1781 | 1” | Nut – lock - slotted | 5.00 |

**U.N.C. (Unified National Coarse)**

(Pitch angle 60 degrees)

|  |  |  |  |
| --- | --- | --- | --- |
| **Code** | **Diameter & length** | **Item** | **Price** |
|  |  |  |  |
| 1720 | “1/64”(1G x 64 tpi) | Screw – ch-h – slot ted- stainless | 0.30 |
|  |  |  |  |
| 0875 | “4/40” (4G x 40 tpi) x 5/16 | Screw – roundhead – slotted – cad plated | 0.30 |
|  |  |  |  |
| 0859 | “6/32” (6G x 32 tpi)  x ¼ | Screw – panhead – Phillips | 0.30 |
| 0876 | “6/32” (6G x 32 tpi)  x 3/8 | Screw – panhead – Phillips | 0.30 |
| 0798 | “6/32” (6G x 32 tpi)  x ½ | Screw – csk – Phillips – zincchromate | 0.30 |
| 1556 | “6/32” (6G x 32 tpi)  x ½ | Screw – csk – slotted - stainless | 0.60 |
| 0613 | “6/32” (6G x 32tpi)  x 2 | Screw – panhead – Phillips – black | 0.30 |
| 0454 | “6/32” (6G x 32 tpi)  x 2 | Screw – roundhead – cad plated | 0.30 |
| 0868 | “6/32” (6G x 32tpi) | Nut – self-locking | 0.05 |
| 1557 | “6/32” (6G x 32 tpi) | Nut - stainless | 0.30 |
| 0609 | “8/32” (8G x 32tpi)  x 5/16 | Screw – csk – Phillips – zinchrom | 0.30 |
| 1305 | “8/32” (8G x 32tpi)  x 1/2 | Screw – roundhead – slottd - stainless | 0.60 |
| 0611 | “8/32” (8G x 32tpi)  x 1 | Screw – panhead – Phillips – znchromate or zinc | 0.30 |
|  |  |  |  |
|  | **¼” UNC** |  |  |
| 0589 | ¼ x ¾ | Bolt – TL ½” , drilled head, zinc chromate plated | 0.30 |
| 1608 | ¼ | Nut – nylock - zincchromate | 0.50 |
|  | **5/16” UNC** |  |  |
| 0880 | 5/16 x 1 | Bolt and nut – HT (Grade 5) | 0.50 |
| 1095 | 5/16 X 1 | Setscrew – HT (Grade 5) – cadpl | 0.30 |
| 1634 | 5/16 x 2 | Screw – roundhead – slot - | 0.50 |
|  |  |  |  |
|  | **3/8” UNC** |  |  |
| 0795 | 3/8 X 1 ½ | Bolt – HT (Grade5) – TL 1”  And nut | 1.00 |
| 0791 | 3/8 x 2 | Bolt - HT (Grade 5) and nut | 1.00 |
| 0796 | 3/8 | Nut – HT | 0.50 |
|  |  |  |  |
|  | **½” UNC** |  |  |
| 0515 | ½ x ¾ | Grubscrew – square head | 1.50 |
| 0453 | ½ x 1 | Grubscrew – square head | 1.50 |
| 0672 | ½ x 3 | Stud – Grade B7 | 2.00 |
| 1639 | ½ x 3 3/8 | Bolt – Newall HT | 2.00 |
| 1638 | ½ x 4 ½ | Bolt – Newall HT | 3.00 |
| 0887 | ½ x 5 | Capscrew | 2.00 |
| 1303 | ½ | Nut – HT - black | 1.00 |
| 0441 | ½ | Nut – split thread lock (“Aerotight’) | 1.00 |
| 1560 | ½ | Nut – plain - zinc-chromate | 1.50 |
|  |  |  |  |
|  | **9/16” UNC** |  |  |
| 1643 | 9/16 x 2 ½ | Bolt - black | 2.00 |
| 1644 | 9/16 x 3 | Bolt – black – head drilled | 2.00 |
|  |  |  |  |
|  |  |  |  |
|  | **5/8” UNC** |  |  |
| 1251 | 5/8 x 2 1/2 | Stud – fully threaded - Grade B7 | 2.00 |
| 1252 | 5/8 x 4 | Stud – fully threaded - Grade B7 | 4.00 |
|  |  |  |  |
|  | **¾” UNC** |  |  |
| 1253 | ¾ x 4 | Stud – fully threaded – Grade B7 | 5.00 |
| 1254 | ¾ x 4 | Stud – fully thread – Grade B8M | 10.00 |
| 1257 | ¾ | Nut – Grade B8M | 6.00 |

**U.N.8 (Unified National 8 TPI)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Code** | **Diameter & length** | **Item** | **Price** |
|  | **1 1/8” UN8** |  |  |
| 1255 | 1 1/8 x 6 | Stud – Grade B8M | 30.00 |
| 1256 | 1 1/8 | Nut - | 10.00 |
|  |  |  |  |
|  | **1 ¼” UN8** |  |  |
| 1258 | 1 ¼ x 7 1/2 | Stud – Grade BM8 | 50.00 |
| 1259 | 1 ¼ | Nut – Grade 8MA | 10.00 |

**Brass Thread (BSB)**

**(26 TPI all diameters – Pitch Angle 55 degrees)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Code** | **Diameter & Length** | **Item** | **Price** |
| 0600 | 3/8 | Nut – brass | 0.60 |
| 0521 | 5/8 | Dome / Acorn Nuts | 4.00 |

**Cycle Thread**

**(“BSCY” - 26 TPI OR 20 TPI – Pitch Angle 60 degrees)**

|  |  |  |  |
| --- | --- | --- | --- |
| **Code** | **Diameter & Length** | **Item** | **Price** |
| 1526 | ¼ X 26TPI | Nut – plain hex - zinc plated | 0.60 |
|  |  |  |  |
| 1282 | 5/16 x ¾ x 26 TPI | Setscrew – mild - zinc plated | 2.50 |
| 0856 | 5/16 x 1 X 26 TPI | Setscrew – zinc plated | 2.50 |
| 0596 | 5/16 X 26 TPI | Nut – plain hex – zincpl | 1.00 |
| 1994 | 5/16 x 26 TPI | Nut – reduced hex - .250 hi | 1.50 |
|  |  |  |  |
| 1881 | 3/8 X 1 | Setscrew - zincplated | 3.50 |
| 1114 | 3/8 X 26 TPI | Nut – plain hex – zincpl | 1.50 |
|  |  |  |  |
| 1115 | 7/16 X 26 TPI | Nut – plain hex – zincpl | 2.20 |
| 1595 | 7/16 X 20 TPI | Nut – plain hex - zincpl | 2.50 |
|  |  |  |  |
| 1596 | ½” X 20 TPI | Nut – plain hex - zincpl | 2.60 |
| 1597 | ½” x 26 TPI | Nut – plain hex – satinchrome | 3.50 |
| 1992 | ½ x 26 TPI | Nut – plain hex - zincplated | 3.00 |

**Metric**

|  |  |  |  |
| --- | --- | --- | --- |
| **Code** | **Diameter & Length** | **Item** | **Price** |
| 1955 | M3 X 16mm | Socket head capscrew stainless | 1.00 |
| 1956 | M3 | Nuts - stainless | 0.30 |
| 1953 | M4 X 16 mm | Socket head capscrew - stainless | 1.00 |
| 1954 | M4 | Nuts - stainless | 0.50 |
| 0670 | M5 x 65mm | Screw – socket head | 0.60 |
| 0612 | M5 | Nut – nylock | 0.30 |
| 1355 | M6 X 16mm | Setscrew - stainless | 0.50 |
| 1584 | M6 X 30 MM | Screw – panhead Phillips - stainless | 1.00 |
| 0712 | M6 | Spring washer – zinc plated | 0.30 |
| 1356 | M6 | Nut - stainless | 0.30 |
| 1179 | M8 x 25mm (1.25 pitch) | Bolt – flanged – zincchromate | 0.30 |
| 0614 | M8 x 40 mm (1.25 pitch) | Bolt + nut – zinc plated | 0.60 |
| 0799 | M8 | Nut – with flange – plated | 0.30 |
| 0976 | M8 | Nylock Nut | 0.50 |
| 1968 | M8 | Dome nut – 1.25 pitch - stainless | 1.00 |
| 0969 | M10 x 40 | Setscrew – socket head | 0.50 |
| 0878 | M10 x 170mm (1.5 p) | Bolt and nut | 1.00 |
| 0931 | M10 | Nylock nut | 0.50 |
| 1628 | M10 | Dome nut - chrome | 3.00 |
| 1980 | M10 | Nut - stainless | 1.00 |
| 0610 | M12 x 25mm (1.75 pitch=coarse) | Capscrew – HT – zinchrom plated | 0.60 |
| 1768 | M12 x 25mm (1.75 pitch=coarse) | Button-head bolt – socket drive - black | 0.50 |
| 0884 | M12 x 75 (1.5 p) | Bolt – TL 25mm – zincchromate | 0.50 |
| 1986 | M14 (1.0 P) | Nut- stainless – 1.0 pitch | 3.00 |
| 0893 | M14 x 55 (2.0 p) | Bolt and nut – HT (class 8.8) | 3.00 |
| 0700 | M16 x 30mm | Setscrew – stainless | 4.00 |
| 0889 | M16 x 80 mm(1.5 p) | Bolt | 2.00 |
| 0888 | M16 x 110 (1.5 p) | Bolt | 3.00 |
| 0890 | M16 x 125 mm (1.5 p) | Bolt | 3.00 |
| 0699 | M16 | Nut – stainless, plus lockwashers | 2.00 |
| 0886 | M18 x 60 mm (1.5 p) | Bolt | 1.50 |

**Mixed-Thread Studs**

|  |  |  |
| --- | --- | --- |
| **Code** | **Diameter/s & Thread type and Lengths and overall length** | **Price** |
| 1042 | (¼UNF TL ½) x (5/16 WHIT TL 3/8) x 1 ¼ | 1.00 |
| 1043 | ¼ x 1 3/8 - (WHIT TL ½) x (BSF TL ¾) | 1.50 |
| 1044 | 5/16 x 2 - (UNC TL 5/8) x (UNF TL 1”) | 2.00 |
| 1045 | 5/16 x 5 ¼ (UNF TL ½) x (WHIT TL ¾) | 5.00 |
| 1988 | ½” x 1 5/8” (UNF TL ½”) X (UNC TL ¾”) | 5.00 |
| 1046 | 7/16 x 3 ¼ - (WHIT TL ¾) x (UNF TL ¾) | 6.50 |
| 1047 | 7/16 x 3 ¾ - (WHIT TL ¾) x (UNF TL 1 ¼ ) | 6.60 |
| 1049 | 7/16 x 4 - (WHIT TL ¾) x (UNF TL 5/8 ) | 8.00 |

**Self-Tappers**

|  |  |  |  |
| --- | --- | --- | --- |
| **Code** | **Diameter & Length** | **Item** | **Price** |
| 1737 | 0g/48 x 3/16 | Screw – roundhead – slot - | 0.50 |
|  |  |  |  |
| 1019 | 4g x ½ | Screw – csk – slotted - stainless | 0.30 |
|  |  |  |  |
| 1162 | 4g x ½ | Screw – raised csk – slotted - stainless | 0.30 |
| 1983 | 4g x 1/2 | Screw – raised csk – slotted – steel nickel plated | 0.60 |
| 0783 | 4g x ½ | Screw – panhead – slotted – stainless | 0.30 |
| 1020 | 4g x ¾ | Screw – csk – slotted - stainless | 0.30 |
| 1667 | 6g x 3/8 | Screw – panhead – slotted - zplated | 0.30 |
| 1155 | 6g x ½ | Screw – raised csk - slotted - cad | 0.30 |
| 1974 | 6g x ½ | Screw – raised csk – slotted - stainless | 0.40 |
| 1154 | 6g x 5/8 | Screw – raised csk – slotted | 0.30 |
| 0994 | 6g x ¾ | Screw – raised csk slotted stainless | 1.00 |
| 1290 | 6g x ¾ | Screw – panhead slotted stainless | 0.50 |
| 1069 | 6g x 1 | Screw – raised csk slotted stainless | 0.50 |
| 1670 | 6g x 1 ¼ | Screw – raised csk slotted stainless | 0.60 |
| 1975 | 8g x 3/8 | Screw – raised csk slotted stainless | 0.40 |
| 1143 | 8g x ½ | Screw – csk – Phillips - chrome | 0.30 |
| 1675 | 8g x ½ | Screw – raised csk – slot - stainless | 0.50 |
| 0995 | 8g x ¾ | Screw – raised csk slotted stainless | 0.50 |
| 1021 | 8g x 1 | Screw – csk – slotted - stainless | 0.60 |
| 1633 | 8g x 1 | Screw – panhead – slotted - zplated | 0.30 |
| 1070 | 8g x 1 | Screw – raised csk slotted stainless | 0.60 |
| 1533 | 8g x 1 1/2 | Screw – csk – stainless - slotted | 0.60 |
|  |  |  |  |
| 1157 | 10g x 5/8 | Screw – csk - slotted | 0.30 |
| 1000 | 10g x ¾ | Screw – raised csk slotted stainless | 0.60 |
| 1022 | 10g x 1 | Screw – csk – slotted - stainless | 0.60 |
| 1976 | 10g x 1 | Screw – raised csk slotted stainless | 0.70 |

Flat Washers

|  |  |  |  |
| --- | --- | --- | --- |
| Code | Diameter | Item | Price |
| 1721 | M 1.6 | Flat washer - stainless | 0.30 |
| 1722 | M 2 | Flat washer - stainless | 0.30 |
|  |  |  |  |
|  |  |  |  |
| 1026 | 6 BA x 24 g | Flat steel washer – zinc plated | 0.30 |
| 1957 | M3 X 7mm X 0.5 | Flat washer - stainless | 0.30 |
| 0857 | 1/8 | Flat washer – stainless | 0.30 |
| 1025 | 1/8 | Flat steel washer – zinc plated | 0.30 |
| 1411 | 1/8 | Flat brass washer | 0.30 |
| 1991 | 5BA | Flat brass washer | 0.40 |
| 1410 | 4BA | Flat brass washer | 0.30 |
| 1409 | 5/32 | Flat brass washer | 0.30 |
| 1006 | 4 mm / 3BA | Flat stainless washer | 0.25 |
| 1024 | 4 mm / 3 BA | Flat steel washer – zinc plated | 0.30 |
| 1023 | 2BA x 20 g | Flat steel washer – zinc plated | 0.30 |
| 1802 | 2BA – o/d 9.75 mm | Flat washer - stainless | 0.50 |
| 1803 | 2BA – o/d 12.65 mm | Flat washer – stainless | 0.60 |
| 0874 | 3/16 i/d x 7/16 o/d x 20g | Flat steel washer - unplt | 0.30 |
| 1993 | 3/16 i/d x 7/16 o/d x 20g | Flat steel washer – zinc plt | 0.50 |
| 0531 | 3/16 i/d x 7/16 o/d x 20g | Flat stainless washer | 0.30 |
| 0592 | 3/16 i/d x 7/16 o/d  x 1/16 | Flat aluminium washer | 0.15 or $5 per 100 |
| 1003 | 3/16 i/d x 7/16 o/d | Flat brass washer | 0.30 |
| 0984 | 3/16 i/d x ½ o/d  x 1/16 | Flat steel washer – zincchromate | 0.30 |
| 0871 | M6 / 0 BA | Flat washer | 0.30 |
| 0883 | ¼ i/d x ½ o/d x 20g | Flat steel washer in Lucas bag | 0.30 |
| 0980 | ¼ i/d x ½ o/d x 20g | Flat stainless washer | 0.30 |
| 1004 | ¼ i/d x 5/8 | Flat brass washer | 0.50 |
| 0532 | ¼ x ¾ o/d x 16g | Flat zinc plated washer | 0.30 |
| 0607 | ¼ i/d x 1 ¼ o/d | Mudguard washer – zincpl – 16g | 0.30 |
| 0863 | 5/16 x 5/8 o/d | Flat washer – dark zincchromate | 0.30 |
| 0979 | 5/16 i/d x ¾ o/d  x 16g | Flat washer - zinc plated | 0.30 |
| 0533 | 5/16 i/d x 7/8 o/d  x 14g | Flat zinc plated washer | 0.30 |
| 0989 | 5/16 i/d x 1 ¼ o/d  x 16g | Flat washer – Mudguard washer - zinc plated | 1.00 |
| 0982 | 3/8 i/d x ¾ ” o/d  x 3 mm | Flat washer | 0.30 |
| 1668 | 3/8 x ¾ x 18g | Flat washer zinc plated | 0.30 |
| 1544 | 3/8 x 7/8 x 16 g | Flat washer zinced | 0.30 |
| 0534 | 3/8 i/d x 1” o/d  x 3 mm | Flat zinc plated washer | 0.30 |
| 1916 | 3/8 x 1 3/16 x 1 mm | Flat stainless washer | 0.50 |
| 1677 | 10 mm x 20 mm x 1.2 - | Flat washer - stainless | 0.50 |
| 0983 | 7/16 i/d x 7/8 o/d x 16g | Flat washer | 0.30 |
| 0535 | 7/16 i/d x 7/8 o/d x 16g | Flat zinc plated washer | 0.30 |
| 2003 | 7/16 i/d x 1” o/d x 16g | Flat zinc plated washer | 0.40 |
| 0985 | 1/2 i/d x 7/8 o/d  x 0.5mm | Flat washer / shim – zincchromate plated | 0.30 |
| 0981 | ½ i/d x 1” o/d x 16g | Flat washer unplated | 0.30 |
| 1545 |  |  |  |
| 0978 | ½ i/d x 1” o/d x 16g | Flat zinc plated washer | 0.30 |
| 1884 | ½ i/d x 1 ¼ o/d | Flat washer - stainless | 0.50 |
| 0536 | ½ i/d x 1 3/8 o/d x 3 mm | Flat zinc plated washer | 0.30 |
| 1774 | ½ i/d x 2? o/d x 12g | Flat zinced washer | 1.00 |
| 0583 | 5/8 i/d x 1 1/16 o/d | Flat washer – zincchromate | 0.30 |
| 0537 | 5/8 i/d x 1 ¼ o/d x 14g | Flat zinc plated washer | 0.30 |
| 1995 | 5/8 i/d x 1 ¼ o/d x 16g | Flat washer - stainless | 2.00 |
|  |  |  |  |
| 0988 | ¾ i/d x 1 1/8 o/d x 14g | Flat washer | 0.30 |
| 0538 | ¾ i/d x 1 ½ o/d x 14g | Flat zinc plated washer | 0.30 |
| 0986 | 13/16 i/d x 1 5/16 o/d x 16g | Flat washer | 0.30 |
| 0987 | 13/16 i/d x 1 5/16 o/d x 16g | Flat washer | 0.30 |
| 0539 | 7/8 | Flat zinc plated washer | 0.30 |
| 0540 | 1 | Flat zinc plated washer | 0.30 |
| 0591 | 1.0 i/d x 1 9/16 o/d x 0.9 mm thick | Flat steel washer | 0.30 |

**Spring Washers**

|  |  |  |  |
| --- | --- | --- | --- |
| **Code** | **Inside Diameter** | **Item** | **Price** |
| 1428 | 1/8 | Spring Washer – zinc plated | 0.30 |
| 1555 | 1/8 6g | Spring washer - stainless | 0.30 |
| 1786 | 5/32 (3BA) | Spring Washer - stainless | 0.30 |
| 0541 | 3/16 | Spring washer – zinc plated | 0.50 |
| 1960 | 3/16 | Spring washer - zinchromate | 0.50 |
| 1002 | 3/16 ( or 10g or 2BA) | Spring washer – stainless steel | 0.30 |
| 0542 | ¼ | Spring washer – zinc plated | 0.30 |
| 1009 | ¼ | Spring washer – plain - cadpl. | 0.30 |
| 1592 | ¼ | Spring washer - stainless | 0.50 |
| 1961 | ¼ | Spring washer - zinchromate | 0.60 |
| 0543 | 5/16 | Spring washer – zinc plated | 0.60 |
| 1962 | 5/16 | Spring washer - zinchromate | 0.70 |
| 0581 | 5/16 | Spring washer – Grover style cadpl. | 1.00 |
| 1787 | 5/16 | Spring washer - stainless | 0.60 |
| 0544 | 3/8 | Spring washer – round edge - zinc plated | 0.50 |
| 1905 | 3/8 | Spring washer – imperial square cut - zincplated | 0.50 |
| 1963 | 3/8 | Spring washer - zinchromate | 0.50 |
| 0545 | 7/16 | Spring washer – zinc plated | 1.50 |
| 1964 | 7/16 | Spring washer - zinchromate | 1.00 |
| 0546 | ½ | Spring washer – flat section - zinc plated | 0.50 |
| 1965 | ½ | Spring washer - zinchromate | 0.60 |
| 0865 | ½ | Spring washer – square section - unplated | 0.50 |
| 0547 | 5/8 | Spring washer – zinc plated | 0.50 |
| 1996 | 5/8 | Spring Washer - stainless | 1.50 |
| 0548 | ¾ | Spring washer – zinc plated | 1.00 |
| 0549 | 7/8 | Spring washer – zinc plated | 1.00 |

**Miscellaneous Washers**

|  |  |  |  |
| --- | --- | --- | --- |
| **Code** | **Inside Diameter** | **Item** | **Price** |
| 1435 | 6 BA | Thackeray Washer | 0.50 |
| 1205 | 4g | Cup washer – nickel plated brass | 0.30 |
| 0996 | 6g | Cup washer – nickel plated brass | 0.30 |
| 1071 | 6g | Cup washer – flanged – stainless | 0.30 |
| 1979 | 6g | Cup washer – non-flanged – stainless | 0.30 |
| 1111 | 6g | Countersunk Trim Washer – brass – nickel plated | 0.30 |
| 1434 | 4 BA | Thackeray Washer – cad plated | 0.50 |
| 1433 | 3 BA | Thackeray Washer – cad plated | 0.50 |
| 1440 | 3 BA | Thackeray Washer - copper | 0.60 |
| 0997 | 8g | Cup washer – nickel plated brass | 0.30 |
| 1072 | 8g | Cup washer – flanged – stainless | 0.50 |
| 1112 | 8g | Countersunk Trim Washer – brass – nickel plated | 0.30 |
| 1439 | 2 BA | Thackeray (double-coil) washer - cad plated | 0.50 |
| 0809 | 3/16 / 10g | Plain Cone (shallow csk) Washer | 0.50 |
| 1050 | 3/16 | Thackeray (double coil) washer– unplated | 0.50 |
| 0998 | 10g | Cup washer – nickel plated brass | 0.50 |
| 1113 | 10g | Countersunk Trim Washer – brass – nickel plated | 0.50 |
|  |  |  |  |
| 1978 | 12g | Cup washer – nickel plated brass | 0.60 |
|  |  |  |  |
| 0804 | ¼ | Floorboard Washer – zinc plated | 1.40 |
| 0867 | ¼ | Washer – external star – zinchrome | 0.05 |
| 0805 | ¼ / 12g | Countersunk Trim Washer – brass – nickel plated | 0.60 |
| 1052 | ¼ | Thackeray (double-coil) washer - unplated | 0.50 |
| 0963 | ¼ | Thackeray (double-coil) washer - zinc plated | 0.50 |
| 1436 | ¼ | Thackeray (double-coil) washer - cad plated | 0.50 |
| 0810 | 5/16 | Thackeray (double-coil) washer- zinc plated | 0.50 |
| 0811 | 3/8 | Thackeray (double-coil) washer- zinc plated | 1.00 |
| 1408 | 3/8 | Thackeray (double-coil) washer- black | 1.00 |
| 1437 | 3/8 | Thackeray (double-coil) washer – cad plated | 1.00 |
| 1189 | 7/16 | Thackeray (double-coil) washer- zinc plated | 1.00 |
| 1438 | 7/16 | Thackeray (double-coil) washer – cad plated | 1.00 |
| 1190 | ½ | Thackeray (double-coil) washer- zinc plated | 1.50 |
| 1373 | ½ | Thackeray (double-coil) washer- unplated – extra wide | 2.00 |
| 1374 | 9/16 | Thackeray (double-coil) washer- cad plated | 2.50 |
| 1316 | 5/8 | Thackeray (double-coil) washer- cad plated | 3.00 |

**Clevis Pins**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Code** | **Diam** | **Length from under head to start hole** | **Length from under head to end of pin** | **Price** |
| 0630 | 3/16 | 5/8” | ¾” | 1.50 |
| 0631 | ¼ | 11/16” | ¾” | 1.70 |
| 1924 | ¼ | ¾” | 7/8” | 2.00 |
| 0632 | ¼ | 7/8” | 1” | 2.00 |
| 1925 | ¼ | 1” | 1 1/8” | 2.20 |
| 0641 | 9/32 | ½” | 5/8” | 2.50 |
| 0640 | 5/16 | ½” | 5/8” | 2.50 |
| 0633 | 5/16 | 5/8” | ¾” | 2.80 |
| 0639 | 5/16 | ¾” | 7/8” | 2.00 |
| 1926 | 5/16 | ¾” | 15/16” | 3.00 |
| 0634 | 5/16 | 1” | 1 ¼” | 3.20 |
| 0642 | 11/32 | ½” | 5/8” | 3.50 |
| 0637 | 3/8 | ¾” | 7/8” | 3.80 |
| 0638 | 3/8 | 1 1/8” | 1 ¼” | 4.00 |
| 1927 | 3/8 | 1 ¼” | 1 3/8” | 4.20 |
| 0635 | ½ | 1” | 1 ¼” | 5.00 |
| 0636 | 5/8 | 1 1/8” | 1 3/8” | 6.00 |

**Split Pins**

|  |  |  |  |
| --- | --- | --- | --- |
| **Code** | **Diameter x Length** | **Item** | **Price** |
| 0777 | 1/32 x ½ (overall) | Split pin – stainless | 0.30 |
| 0778 | 3/64 x ½ (overall) | Split pin | 0.30 |
| 0779 | 1/16 x 1” (overall) | Split pin | 0.30 |
| 0713 | 1/8 x 1¼ (1¾ overall)  = 3.2 mm x 45 mm | Split pin – stainless steel | 0.50 |

**BSF TAPS**

|  |  |  |  |
| --- | --- | --- | --- |
| **Code** | **Diameter** | **Item** | **Price** |
| 0733 | 3/16 | Tap – RHT – Inter - carbon | $8.00 |
| 1075 | 3/16 | Tap – RHT – Taper - HSS | $15.00 |
| 1030 | 3/16 | Tap – RHT – Inter - HSS | $15.00 |
| 1076 | 3/16 | Tap – RHT – Bottom - HSS | $15.00 |
| 1074 | 3/16 | Taps – RHT – set of 3 – HSS | $25.00 |
|  |  |  |  |
| 1171 | 7/32 | Tap – RHT – interm. | $25.00 |
|  |  |  |  |
| 0734 | ¼ | Tap – RHT – Bottoming | $20.00 |
| 1077 | ¼ | Taps – RHT – set of 3 – HSS | $40.00 |
| 1029 | ¼ | Tap – LHT | $25.00 |
| 1931 | ¼ | Tap – RHT - taper | 30.00 |
|  |  |  |  |
| 0735 | 9/32 | Tap – RHT – bottoming | $25.00 |
|  |  |  |  |
| 1080 | 5/16 | Tap – RHT – Taper – HSS | $25.00 |
| 1031 | 5/16 | Tap – RHT – intermediate | $25.00 |
| 0736 | 5/16 | Tap – RHT – bottoming – carbon steel | $25.00 |
|  |  |  |  |
| 1032 | 3/8 | Tap – RHT – Taper – ch/alloy | $38.00 |
| 1561 | 3/8 | Tap – RHT – Interm – Carbon steel | $38.00 |
| 1893 | 3/8 | Tap – RHT – bottom – carbon steel | $28.00 |
| 0738 | 3/8 | Tap - RHT – bottom – HSS | $30.00 |
| 1892 | 3/8 | Tap – RHT – bottom – P and N chrome steel | $32.00 |
| 1950 | 3/8 | Taps – set of 3 – carbon steel | $35.00 |
| 0737 | 3/8 | Tap – LHT | $35.00 |
| 1079 | 3/8 | Tap – LHT – HSS | $45.00 |
|  |  |  |  |
| 1494 | 13/32 | Tap - Interm | $35.00 |
| 1495 | 13/32 | Tap - Taper | $35.00 |
|  |  |  |  |
| 1033 | 7/16 | Tap – RHT – taper | $30.00 |
| 0785 | 7/16 | Tap – RHT – bottoming | $30.00 |
| 1949 | 7/16 | Taps – set of 3 – carbon steel | $35.00 |
| 1027 | 7/16 | Tap – LHT | $35.00 |
|  |  |  |  |
| 0040 | ½ | Tap – RHT – Taper – HSS | $35.00 |
| 0039 | ½ | Tap – RHT – Interm – HSS | $35.00 |
| 0740 | ½ | Tap – RHT – Bottom – HSS | $35.00 |
| 0739 | ½ | Tap – LHT **-** Bottom - HSS | $35.00 |
|  |  |  |  |
| 0741 | 9/16 | Tap – RHT – bottoming | $30.00 |
| 1082 | 9/16 | Tap – RHT – bottom – HSS | $70.00 |
| 1078 | 9/16 | Tap – LHT – HSS | $40.00 |
|  |  |  |  |
| 0742 | 5/8 | Tap – RHT – intermediate | $35.00 |
| 0041 | 5/8 | Tap – RHT – Bottom – HSS | $35.00 |
| 0056 | 5/8 | Tap – LHT – Interm – HSS | $35.00 |
|  |  |  |  |
| 0743 | 11/16 | Tap – RHT – bottoming | $45.00 |
|  |  |  |  |
| 0744 | ¾ | Tap – RHT – bottoming | $50.00 |
| 1611 | ¾ | Tap – LHT - bottoming | $40 |
|  |  |  |  |
|  |  |  |  |
| 0745 | 13/16 | Tap – RHT – Taper- HSS | $50.00 |
| 0047 | 13/16 | Tap – RHT – Interm-HSS | $50.00 |
| 0048 | 13/16 | Tap – RHT – Bottom – HSS | $50.00 |
|  |  |  |  |
| 0746 | 7/8 | Tap – RHT – Interm | $55.00 |
|  |  |  |  |
| 0747 | 15/16 | Tap – RHT – Interm | $55.00 |
|  |  |  |  |
| 0748 | 1 | Tap – RHT – Bottom – HSS | $60.00 |
|  |  |  |  |
| 0749 | 1 1/8 | Tap – RHT – Interm | $65.00 |
| 0750 | 1 ¼ | Tap- RHT – Interm | $65.00 |
| 0751 | 1 ½ | Tap – RHT – Bottoming | $70.00 |

**BSF BUTTON DIES**

|  |  |  |  |
| --- | --- | --- | --- |
| **Code** | **Diameter** | **Item** | **Price** |
| 0753 | 3/16 x 1” o/d | Die – RHT | $35.00 |
| 1170 | 7/32 x 1” o/d | Die – RHT | $30.00 |
| 1317 | 7/32 x 1” o/d | Die - LHT | $40.00 |
| 1274 | ¼ x 1” o/d | Die - RHT | $30.00 |
| 0754 | ¼ x 1 ½” o/d | Die - RHT | $70.00 |
| 0755 | 9/32 x 1½” o/d | Die - RHT | $30.00 |
| 1392 | 5/16 X 1”od | Die - RHT | $35.00 |
| 0756 | 5/16 x 1½ o/d | Die - RHT | $30.00 |
| 0757 | 3/8 x 1” o/d | Die - RHT | $30.00 |
| 1496 | 3/8 x 1 ½ o/d | Die - RHT | $70.00 |
| 0758 | 7/16 x 1” o/d | Die - RHT | $35.00 |
| 1393 | 7/16 x 1 ½” od | Die - RHT | $35.00 |
| 0759 | ½ x 1½” o/d | Die - RHT | $35.00 |
| 1502 | ½ x 2” od | Die - RHT | $40.00 |
| 0761 | 9/16 x 2” o/d | Die - RHT | $40.00 |
| 0760 | 9/16 | Die - **LHT** | $40.00 |
| 1497 | 5/8 X 1 ½ | Die - RHT | $40.00 |
| 0762 | 5/8 x 2” o/d | Die - RHT | $45.00 |
| 0763 | 11/16 x 2” od | Die - RHT | $50.00 |
| 0764 | ¾ x 2” od | Die - RHT | $55.00 |
| 0765 | 13/16 x 2” o/d | Die - RHT | $55.00 |
| 0766 | 7/8 x 2” o/d | Die - RHT | $60.00 |
| 0767 | 15/16 x 2” o/d | Die - RHT | $60.00 |
| 0768 | 1 x 2” o/d | Die - RHT | $60.00 |

**BSF DIE NUTS**

|  |  |  |  |
| --- | --- | --- | --- |
| **Code** | **Diameter** | **Item** | **Price** |
| 1275 | 3/16 | Die Nut | 30.00 |
| 1276 | 1/4 | Die Nut carbon s | 35.00 |
| 1277 | 5/16 | Die Nut | 35.00 |
| 1278 | 3/8 | Die Nut | 35.00 |
| 1377 | 7/16 | Die Nut | 40.00 |
| 1378 | 1/2 | Die nut | 40.00 |
| 1911 | 13/16 | Die Nut | 55.00 |
| 1921 | 1” | Die Nut | 65.00 |

**B.A. TAPS**

|  |  |  |  |
| --- | --- | --- | --- |
| **Code** | **Diameter** | **Item** | **Price** |
| 0060 | 0 BA | Tap – taper – long-HSS | 10.00 |
| 0073 | 0 BA | Tap – taper – HSS | 10.00 |
| 0080 | 0 BA | Tap – interm – HSS | 10.00 |
| 1600 | 0 BA | Taps – set of 3 - HSS | 25.00 |
|  |  |  |  |
|  |  |  |  |
| 0084 | 1 BA | Tap – taper – HSS | 10.00 |
| 0088 | 1 BA | Tap – interm – HSS | 10.00 |
| 0090 | 1 BA | Tap – bottom – HSS | 10.00 |
| 0092 | 1 BA | Tap – set of 3 – HSS | 25.00 |
|  |  |  |  |
| 0093 | 2 BA | Tap – taper – HSS | 10.00 |
| 0095 | 2 BA | Tap – interm – HSS | 10.00 |
| 0096 | 2 BA | Tap – bottom – HSS | 10.00 |
| 0101 | 2 BA | Tap – interm – LHT – HSS | 15.00 |
| 1601 | 2 BA | Taps – set of 3 - HSS | 25.00 |
|  |  |  |  |
|  |  |  |  |
| 0104 | 3 BA | Tap – taper – HSS | 10.00 |
| 0108 | 3 BA | Tap – interm – HSS | 10.00 |
| 0112 | 3 BA | Tap – bottom – HSS | 10.00 |
| 0115 | 3 BA | Taps – set of 3 – HSS | 25.00 |
|  |  |  |  |
| 0123 | 4 BA | Tap – taper | 10.00 |
| 0141 | 4 BA | Tap – interm – HSS | 10.00 |
| 0142 | 4 BA | Tap – bottom – HSS | 10.00 |
| 0146 | 4 BA | Tap – interm – LHT – HSS | 15.00 |
|  |  |  |  |
| 0148 | 5 BA | Tap – taper | N/a |
| 0150 | 5 BA | Tap – interm – HSS | 10.00 |
| 0153 | 5 BA | Tap – bottom | N/a |
|  |  |  |  |
| 0163 | 6 BA | Tap – taper | N/a |
| 0164 | 6 BA | Tap – interm – HSS | 10.00 |
| 0166 | 6 BA | Tap – bottom – HSS | 10.00 |
|  |  |  |  |
| 0167 | 7 BA | Tap – taper | N/a |
| 0169 | 7 BA | Tap – interm – HSS | 15.00 |
|  |  |  |  |
| 0174 | 8 BA | Tap – taper | N/a |
| 1087 | 8 BA | Tap – interm – HSS | 15.00 |
| 1088 | 8 BA | Taps – set of 3 – HSS | 25.00 |
| 1185 | 10 BA | Tap | 10.00 |

**B.A. BUTTON DIES**

|  |  |  |  |
| --- | --- | --- | --- |
| **Code** | **BA SIZE** | **DIE O/D SIZE** | **Price** |
| 1367 | 0BA | 1” | 35.00 |
| 1368 | 2BA | 1” | 35.00 |
| 2007 | 3BA | 13/16” | 25.00 |
| 1369 | 4BA | 1” | 40.00 |
| 2008 | 5BA | 13/16” | 25.00 |

**WHITWORTH TAPS**

|  |  |  |  |
| --- | --- | --- | --- |
| **Code** | **Diameter** | **Item** | **Price** |
| 0233 | 3/16 | Tap – Taper – HSS | 8.00 |
| 0239 | 3/16 | Tap – Interm – HSS | 8.00 |
| 0244 | 3/16 | Tap – Bottom – HSS | 8.00 |
| 0245 | 3/16 | Taps – set of 3 – HSS | 20.00 |
|  |  |  |  |
| 0228 | 7/32 | Tap – Interm – HSS | 10.00 |
| 0229 | 7/32 | Tap – set of 3 – HSS | 20.00 |
|  |  |  |  |
| 0246 | ¼ | Tap – Interm – HSS | 8.00 |
| 0247 | ¼ | Tap – Bottom – HSS | 8.00 |
|  |  |  |  |
| 0248 | ½ | Tap – Interm – HSS | 15.00 |
| 0249 | ½ | Tap – set of 3 – HSS | 25.00 |
|  |  |  |  |
| 0250 | 7/8 | Tap – Bottom – HSS | 20.00 |
|  |  |  |  |
| 0251 | 1 | Tap – Taper – HSS | 25.00 |
| 0285 | 1 | Tap – Interm – HSS | 25.00 |
| 1093 | 1 | Tap – Bottom – HSS | 25.00 |
|  |  |  |  |
| 1091 | 1 ¼ | Tap – Bottom – HSS | 30.00 |
|  |  |  |  |
| 0158 | 1 3/8 | Tap – Bottom – HSS | 30.00 |
|  |  |  |  |
| 1089 | 1 ½ | Tap – Bottom – HSS | 35.00 |

**UNF TAPS**

|  |  |  |  |
| --- | --- | --- | --- |
| **Code** | **Diameter** | **Item** | **Price** |
| 0177 | 5/16 | Tap – Bottom – HSS | 8.00 |
| 0178 | 5/16 | Tap – Set of 3 – HSS | 25.00 |
|  |  |  |  |
| 0191 | ¾ | Tap – Interm – HSS | 15.00 |
| 0193 | ¾ | Tap – set of 3 – HSS | 25.00 |
|  |  |  |  |
| 0203 | 7/8 | Tap – Taper – HSS | 20.00 |
| 0206 | 7/8 | Tap – Interm – HSS | 20.00 |
| 0210 | 7/8 | Tap – Bottom – HSS | 20.00 |
| 1090 | 7/8 | Tap – set of 3 – HSS | 40.00 |
|  |  |  |  |
| 0216 | 1 1/8 | Tap – Interm – HSS | 20.00 |
| 0227 | 1 1/8 | Tap – Bottom – HSS | 20.00 |

**BRASS THREAD (26 TPI) TAPS**

|  |  |  |  |
| --- | --- | --- | --- |
| **Code** | **Diameter** | **Item** | **Price** |
| 1501 | 9/16 | Tap – RHT - set of 3 | $100.00 |
| 1500 | ¾ | Tap – RHT – set of 3 | $100.00 |
| 1083 | 7/8 | Tap – RHT – Taper – HSS | $25.00 |
| 1084 | 7/8 | Tap – RHT – Inter – HSS | $25.00 |
| 1085 | 7/8 | Tap – RHT – Bottom – HSS | $25.00 |
| 1086 | 7/8 | Tap – RHT – Set of 3 – HSS | $50.00 |
| 1499 | 1 1/8 | Tap - RHT | $52.00 |
| 1498 | 1 ¼ | Tap - RHT | $55.00 |
| 1503 | 1 ¼ | Tap - RHT – Set of 3 | $110.00 |
| 0059 | 1 ½ | Tap – RHT – Bottom – HSS | $60.00 |

**MISCELLANEOUS HARDWARE**

|  |  |  |  |
| --- | --- | --- | --- |
| **Code** | **Dimensions** | **Item** | **Price** |
| 1056 | 1/4 BSF | Straight grease nipple | 2.00 |
| 1063 | 1/8 BSP | Brass buttonhead hexagon grease nipple | 5.00 |
|  |  |  |  |
| 1761 | 1/16” x 5/8” | Spring Pin / Roll Pin | 1.00 |
| 1429 | 2mm x 16 mm | Spring Pin / Roll Pin | 0.50 |
| 1430 | 3mm x 16 mm | Spring Pin / Roll Pin | 0.50 |
| 1431 | ¼” x 1 ½” | Spring Pin / Roll Pin | 1.00 |
| 1432 | 3/8” x 2” | Spring Pin / Roll Pin | 2.00 |
|  |  |  |  |
| 1933 | 1”x .131x .146 | Taper Pin | 1.00 |
| 1934 | 1 3/8 x .315x .341 | Taper Pin | 5.00 |
| 1935 | 2” x .316 x .335 | Taper Pin | 5.00 |
| 1936 | 2” x .255 x .297 | Taper Pin | 5.00 |
| 1937 | 2” x .192 x .233 | Taper Pin | 5.00 |
| 1938 | 2 1/2” x .193 x.240 | Taper Pin | 5.00 |
| 1939 | 2 1/2” x. 190 x.240 | Taper Pin | 5.00 |
| 1940 | 2 1/2” x .201 x.252 | Taper Pin | 5.00 |
| 1941 | 2 1/2” x .195 x.243 | Taper Pin | 5.00 |